--- a/arch/arm/boot/dts/mt7623.dtsi
+++ b/arch/arm/boot/dts/mt7623.dtsi
@@ -949,17 +949,14 @@
 	};
 
 	crypto: crypto@1b240000 {
-		compatible = "mediatek,eip97-crypto";
+		compatible = "inside-secure,safexcel-eip97";
 		reg = <0 0x1b240000 0 0x20000>;
 		interrupts = <GIC_SPI 82 IRQ_TYPE_LEVEL_LOW>,
 			     <GIC_SPI 83 IRQ_TYPE_LEVEL_LOW>,
 			     <GIC_SPI 84 IRQ_TYPE_LEVEL_LOW>,
-			     <GIC_SPI 91 IRQ_TYPE_LEVEL_LOW>,
-			     <GIC_SPI 97 IRQ_TYPE_LEVEL_LOW>;
+			     <GIC_SPI 91 IRQ_TYPE_LEVEL_LOW>;
+		interrupt-names = "ring0", "ring1", "ring2", "ring3";
 		clocks = <&ethsys CLK_ETHSYS_CRYPTO>;
-		clock-names = "cryp";
-		power-domains = <&scpsys MT2701_POWER_DOMAIN_ETH>;
-		status = "disabled";
 	};
 
 	bdpsys: syscon@1c000000 {
