// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "qcom-ipq4019.dtsi"
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/soc/qcom,tcsr.h>

/ {
	model = "MobiPromo CM520-79F";
	compatible = "mobipromo,cm520-79f";

	aliases {
		led-boot = &led_sys;
		led-failsafe = &led_sys;
		led-running = &led_sys;
		led-upgrade = &led_sys;
	};

	soc {
		rng@22000 {
			status = "okay";
		};

		mdio@90000 {
			status = "okay";
			pinctrl-0 = <&mdio_pins>;
			pinctrl-names = "default";
			reset-gpios = <&tlmm 47 GPIO_ACTIVE_LOW>;
			reset-delay-us = <1000>;
		};

		ess-psgmii@98000 {
			status = "okay";
		};

		tcsr@1949000 {
			compatible = "qcom,tcsr";
			reg = <0x1949000 0x100>;
			qcom,wifi_glb_cfg = <TCSR_WIFI_GLB_CFG>;
		};

		tcsr@194b000 {
			compatible = "qcom,tcsr";
			reg = <0x194b000 0x100>;
			qcom,usb-hsphy-mode-select = <TCSR_USB_HSPHY_HOST_MODE>;
		};

		ess_tcsr@1953000 {
			compatible = "qcom,tcsr";
			reg = <0x1953000 0x1000>;
			qcom,ess-interface-select = <TCSR_ESS_PSGMII>;
		};

		tcsr@1957000 {
			compatible = "qcom,tcsr";
			reg = <0x1957000 0x100>;
			qcom,wifi_noc_memtype_m0_m2 = <TCSR_WIFI_NOC_MEMTYPE_M0_M2>;
		};

		usb2@60f8800 {
			status = "okay";

			dwc3@6000000 {
				#address-cells = <1>;
				#size-cells = <0>;

				usb2_port1: port@1 {
					reg = <1>;
					#trigger-source-cells = <0>;
				};
			};
		};

		usb3@8af8800 {
			status = "okay";

			dwc3@8a00000 {
				#address-cells = <1>;
				#size-cells = <0>;

				usb3_port1: port@1 {
					reg = <1>;
					#trigger-source-cells = <0>;
				};

				usb3_port2: port@2 {
					reg = <2>;
					#trigger-source-cells = <0>;
				};
			};
		};

		crypto@8e3a000 {
			status = "okay";
		};

		watchdog@b017000 {
			status = "okay";
		};

		ess-switch@c000000 {
			status = "okay";
		};

		edma@c080000 {
			status = "okay";
		};
	};

	led_spi {
		compatible = "spi-gpio";
		#address-cells = <1>;
		#size-cells = <0>;

		sck-gpios = <&tlmm 40 GPIO_ACTIVE_HIGH>;
		mosi-gpios = <&tlmm 36 GPIO_ACTIVE_HIGH>;
		num-chipselects = <0>;

		led_gpio: led_gpio@0 {
			compatible = "fairchild,74hc595";
			reg = <0>;
			gpio-controller;
			#gpio-cells = <2>;
			registers-number = <1>;
			spi-max-frequency = <1000000>;
		};
	};

	leds {
		compatible = "gpio-leds";

		usb {
			label = "blue:usb";
			gpios = <&tlmm 10 GPIO_ACTIVE_HIGH>;
			linux,default-trigger = "usbport";
			trigger-sources = <&usb3_port1>, <&usb3_port2>, <&usb2_port1>;
		};

		led_sys: can {
			label = "blue:can";
			gpios = <&tlmm 11 GPIO_ACTIVE_HIGH>;
		};

		wan {
			label = "blue:wan";
			gpios = <&led_gpio 0 GPIO_ACTIVE_LOW>;
		};

		lan1 {
			label = "blue:lan1";
			gpios = <&led_gpio 1 GPIO_ACTIVE_LOW>;
		};

		lan2 {
			label = "blue:lan2";
			gpios = <&led_gpio 2 GPIO_ACTIVE_LOW>;
		};

		wlan2g {
			label = "blue:wlan2g";
			gpios = <&led_gpio 5 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};

		wlan5g {
			label = "blue:wlan5g";
			gpios = <&led_gpio 6 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1tpt";
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			gpios = <&tlmm 18 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};
};

&blsp_dma {
	status = "okay";
};

&blsp1_uart1 {
	status = "okay";
};

&blsp1_uart2 {
	status = "okay";
};

&cryptobam {
	status = "okay";
};

&gmac0 {
	nvmem-cells = <&macaddr_art_1006>;
	nvmem-cell-names = "mac-address";
};

&gmac1 {
	nvmem-cells = <&macaddr_art_5006>;
	nvmem-cell-names = "mac-address";
};

&nand {
	pinctrl-0 = <&nand_pins>;
	pinctrl-names = "default";
	status = "okay";

	nand@0 {
		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "SBL1";
				reg = <0x0 0x100000>;
				read-only;
			};

			partition@100000 {
				label = "MIBIB";
				reg = <0x100000 0x100000>;
				read-only;
			};

			partition@200000 {
				label = "BOOTCONFIG";
				reg = <0x200000 0x100000>;
			};

			partition@300000 {
				label = "QSEE";
				reg = <0x300000 0x100000>;
				read-only;
			};

			partition@400000 {
				label = "QSEE_1";
				reg = <0x400000 0x100000>;
				read-only;
			};

			partition@500000 {
				label = "CDT";
				reg = <0x500000 0x80000>;
				read-only;
			};

			partition@580000 {
				label = "CDT_1";
				reg = <0x580000 0x80000>;
				read-only;
			};

			partition@600000 {
				label = "BOOTCONFIG1";
				reg = <0x600000 0x80000>;
			};

			partition@680000 {
				label = "APPSBLENV";
				reg = <0x680000 0x80000>;
			};

			partition@700000 {
				label = "APPSBL";
				reg = <0x700000 0x200000>;
				read-only;
			};

			partition@900000 {
				label = "APPSBL_1";
				reg = <0x900000 0x200000>;
				read-only;
			};

			art: partition@b00000 {
				label = "ART";
				reg = <0xb00000 0x80000>;
				read-only;
			};

			partition@b80000 {
				label = "ubi";
				reg = <0xb80000 0x7480000>;
			};
		};
	};
};

&qpic_bam {
	status = "okay";
};

&tlmm {
	mdio_pins: mdio_pinmux {
		mux_1 {
			pins = "gpio6";
			function = "mdio";
			bias-pull-up;
		};

		mux_2 {
			pins = "gpio7";
			function = "mdc";
			bias-pull-up;
		};
	};

	nand_pins: nand_pins {
		pullups {
			pins =	"gpio52", "gpio53", "gpio58",
				"gpio59";
			function = "qpic";
			bias-pull-up;
		};

		pulldowns {
			pins =	"gpio54", "gpio55", "gpio56",
				"gpio57", "gpio60", "gpio61",
				"gpio62", "gpio63", "gpio64",
				"gpio65", "gpio66", "gpio67",
				"gpio68", "gpio69";
			function = "qpic";
			bias-pull-down;
		};
	};
};

&usb3_ss_phy {
	status = "okay";
};

&usb3_hs_phy {
	status = "okay";
};

&usb2_hs_phy {
	status = "okay";
};

&wifi0 {
	status = "okay";
	qcom,ath10k-calibration-variant = "CM520-79F";
};

&wifi1 {
	status = "okay";
	qcom,ath10k-calibration-variant = "CM520-79F";
};

&art {
	compatible = "nvmem-cells";
	#address-cells = <1>;
	#size-cells = <1>;

	macaddr_art_1006: macaddr@1006 {
		reg = <0x1006 0x6>;
	};

	macaddr_art_5006: macaddr@5006 {
		reg = <0x5006 0x6>;
	};
};
