#include "bcm6358.dtsi"

#include <dt-bindings/input/input.h>

/ {
	aliases {
		led-boot = &led_power_red;
		led-failsafe = &led_power_red;
		led-running = &led_power_red;
		led-upgrade = &led_power_red;
	};

	chosen {
		bootargs = "rootfstype=squashfs,jffs2 noinitrd console=ttyS0,115200";
		stdout-path = "serial0:115200n8";
	};

	gpiokeys: keys {
		compatible = "gpio-keys-polled";
		#address-cells = <1>;
		#size-cells = <0>;
		poll-interval = <20>;

		wlan {
			label = "wlan";
			gpios = <&pinctrl 9 1>;
			linux,code = <KEY_WLAN>;
			debounce-interval = <60>;
		};

		restart {
			label = "restart";
			gpios = <&pinctrl 10 1>;
			linux,code = <KEY_RESTART>;
			debounce-interval = <60>;
		};

		reset {
			label = "reset";
			gpios = <&pinctrl 11 1>;
			linux,code = <KEY_CONFIG>;
			debounce-interval = <60>;
		};
	};

	gpioleds: leds {
		compatible = "gpio-leds";

		dsl_red {
			label = "red:dsl";
			gpios = <&pinctrl 2 1>;
		};

		led_power_red: power_red {
			label = "red:power";
			gpios = <&pinctrl 3 1>;
			default-state = "on";
		};

		lan1_red {
			label = "red:lan1";
			gpios = <&pinctrl 13 1>;
		};

		lan2_red {
			label = "red:lan2";
			gpios = <&pinctrl 22 1>;
		};

		lan3_green {
			label = "green:lan3";
			gpios = <&pinctrl 23 1>;
		};

		lan3_red {
			label = "red:lan3";
			gpios = <&pinctrl 26 1>;
		};

		lan4_green {
			label = "green:lan4";
			gpios = <&pinctrl 27 1>;
		};

		lan4_red {
			label = "red:lan4";
			gpios = <&pinctrl 28 1>;
		};
	};
};

&pflash {
	status = "okay";

	partitions {
		compatible = "fixed-partitions";
		#address-cells = <1>;
		#size-cells = <1>;

		cfe@0 {
			label = "CFE";
			reg = <0x000000 0x020000>;
			read-only;
		};

		linux@20000 {
			label = "linux";
			reg = <0x020000 0xec0000>;
			compatible = "brcm,bcm963xx-imagetag";
		};

		cal_data@ee0000 {
			label = "cal_data";
			reg = <0xee0000 0x100000>;
			read-only;
		};

		nvram@fe0000 {
			label = "nvram";
			reg = <0xfe0000 0x020000>;
		};
	};
};

&uart0 {
	status = "okay";
};
