From 3343551eb8a692aafcbf1a7eaf0b79965aa60ba9 Mon Sep 17 00:00:00 2001
From: Madalin Bucur <madalin.bucur@nxp.com>
Date: Wed, 16 Oct 2019 11:53:54 +0300
Subject: [PATCH] sdk_dpa: align to upstream PHY_INTERFACE_MODE

Signed-off-by: Madalin Bucur <madalin.bucur@nxp.com>
---
 drivers/net/ethernet/freescale/sdk_dpaa/mac.c | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

--- a/drivers/net/ethernet/freescale/sdk_dpaa/mac.c
+++ b/drivers/net/ethernet/freescale/sdk_dpaa/mac.c
@@ -76,7 +76,7 @@ static const char phy_str[][11] = {
 	[PHY_INTERFACE_MODE_RGMII_TXID]	= "rgmii-txid",
 	[PHY_INTERFACE_MODE_RTBI]	= "rtbi",
 	[PHY_INTERFACE_MODE_XGMII]	= "xgmii",
-	[PHY_INTERFACE_MODE_2500SGMII] = "sgmii-2500",
+	[PHY_INTERFACE_MODE_2500BASEX] = "sgmii-2500",
 };
 
 static phy_interface_t __pure __attribute__((nonnull)) str2phy(const char *str)
@@ -103,7 +103,7 @@ static const uint16_t phy2speed[] = {
 	[PHY_INTERFACE_MODE_RGMII_TXID]	= SPEED_1000,
 	[PHY_INTERFACE_MODE_RTBI]	= SPEED_1000,
 	[PHY_INTERFACE_MODE_XGMII]	= SPEED_10000,
-	[PHY_INTERFACE_MODE_2500SGMII] = SPEED_2500,
+	[PHY_INTERFACE_MODE_2500BASEX] = SPEED_2500,
 };
 
 static struct mac_device * __cold
