#include "mt7621.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "elecom,wrc-1167ghbk2-s", "mediatek,mt7621-soc";
	model = "ELECOM WRC-1167GHBK2-S";

	aliases {
		led-boot = &led_power_green;
		led-failsafe = &led_power_green;
		led-running = &led_power_green;
		led-upgrade = &led_power_green;
	};

	leds {
		compatible = "gpio-leds";

		wlan2g {
			label = "white:wlan2g";
			gpios = <&gpio 3 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0radio";
		};

		wlan5g {
			label = "white:wlan5g";
			gpios = <&gpio 4 GPIO_ACTIVE_LOW>;
		};

		led_power_green: power_green {
			label = "green:power";
			gpios = <&gpio 7 GPIO_ACTIVE_HIGH>;
		};

		power_blue {
			label = "blue:power";
			gpios = <&gpio 8 GPIO_ACTIVE_HIGH>;
		};

		wps {
			label = "red:wps";
			gpios = <&gpio 15 GPIO_ACTIVE_HIGH>;
		};

		power_red {
			label = "red:power";
			gpios = <&gpio 16 GPIO_ACTIVE_HIGH>;
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			gpios = <&gpio 13 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};

		wps {
			label = "wps";
			gpios = <&gpio 18 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};
	};
};

&gmac0 {
	nvmem-cells = <&macaddr_factory_e000>;
	nvmem-cell-names = "mac-address";
};

&switch0 {
	ports {
		port@0 {
			status = "okay";
			label = "wan";
			nvmem-cells = <&macaddr_factory_e006>;
			nvmem-cell-names = "mac-address";
		};

		port@1 {
			status = "okay";
			label = "lan4";
		};

		port@2 {
			status = "okay";
			label = "lan3";
		};

		port@3 {
			status = "okay";
			label = "lan2";
		};

		port@4 {
			status = "okay";
			label = "lan1";
		};
	};
};

&spi0 {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <10000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x0 0x30000>;
				read-only;
			};

			partition@30000 {
				label = "u-boot-env";
				reg = <0x30000 0x10000>;
				read-only;
			};

			factory: partition@40000 {
				label = "factory";
				reg = <0x40000 0x10000>;
				read-only;
			};

			partition@50000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x50000 0xf20000>;
			};

			partition@f70000 {
				label = "user_data";
				reg = <0xf70000 0x80000>;
				read-only;
			};

			partition@ff0000 {
				label = "NVRAM";
				reg = <0xff0000 0x10000>;
				read-only;
			};
		};
	};
};

&state_default {
	gpio {
		groups = "i2c", "uart3", "jtag", "wdt";
		function = "gpio";
	};
};

&pcie {
	status = "okay";
};

&pcie0 {
	wifi@0,0 {
		compatible = "mediatek,mt76";
		reg = <0x0000 0 0 0 0>;
		mediatek,mtd-eeprom = <&factory 0x0>;
		nvmem-cells = <&macaddr_factory_e000>;
		nvmem-cell-names = "mac-address";
		mac-address-increment = <1>;
	};
};

&xhci {
	status = "disabled";
};

&factory {
	compatible = "nvmem-cells";
	#address-cells = <1>;
	#size-cells = <1>;

	macaddr_factory_e000: macaddr@e000 {
		reg = <0xe000 0x6>;
	};

	macaddr_factory_e006: macaddr@e006 {
		reg = <0xe006 0x6>;
	};
};
