From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <rafal@milecki.pl>
Subject: [PATCH] mtd: redboot: add of_match_table with DT binding
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

This allows parsing RedBoot compatible partitions for properly described
flash device in DT.

Signed-off-by: Rafał Miłecki <rafal@milecki.pl>
---

--- a/drivers/mtd/parsers/redboot.c
+++ b/drivers/mtd/parsers/redboot.c
@@ -305,6 +305,7 @@ static int parse_redboot_partitions(stru
 
 static const struct of_device_id mtd_parser_redboot_of_match_table[] = {
 	{ .compatible = "redboot-fis" },
+	{ .compatible = "ecoscentric,redboot-fis-partitions" },
 	{},
 };
 MODULE_DEVICE_TABLE(of, mtd_parser_redboot_of_match_table);
