// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "qca955x_dlink_dap-2xxx.dtsi"

/ {
	compatible = "dlink,dap-2660-a1", "qca,qca9557";
	model = "D-Link DAP-2660 A1";

	aliases {
		led-boot = &led_power_green;
		led-failsafe = &led_power_red;
		led-running = &led_power_green;
		led-upgrade = &led_power_red;
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 17 GPIO_ACTIVE_LOW>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_power_red: power_red {
			label = "red:power";
			gpios = <&gpio 14 GPIO_ACTIVE_LOW>;
		};

		led_power_green: power_green {
			label = "green:power";
			gpios = <&gpio 23 GPIO_ACTIVE_LOW>;
			default-state = "on";
		};
	};
};

&partitions {
	partition@70000 {
		label = "firmware";
		reg = <0x70000 0xee0000>;
		compatible = "wrg";
	};

	partition@f50000 {
		label = "dlink";
		reg = <0xf50000 0xa0000>;
		read-only;
	};

	art: partition@ff0000 {
		label = "art";
		reg = <0xff0000 0x10000>;
		read-only;
	};
};

&mdio0 {
	status = "okay";

	phy4: ethernet-phy@4 {
		reg = <4>;
	};
};

&eth0 {
	status = "okay";

	pll-data = <0x82000000 0x80000101 0x80001313>;

	phy-handle = <&phy4>;
	phy-mode = "rgmii-id";

	gmac-config {
		device = <&gmac>;
		rgmii-enabled = <1>;
		rxd-delay = <3>;
		rxdv-delay = <3>;
	};
};

&pcie0 {
	status = "okay";
};
