#
# Copyright (C) 2012-2015 OpenWrt.org
#

. /lib/functions/uci-defaults.sh

board_config_update

case "$(board_name)" in
actiontec,r1000h|\
dynalink,rta770bw|\
dynalink,rta770w|\
netgear,cvg834g|\
netgear,dgnd3700-v2|\
netgear,evg2000|\
t-com,speedport-w-303v|\
t-com,speedport-w-500v)
	ucidef_set_interface_lan "eth0"
	;;
adb,a4001n1|\
adb,a4001n|\
adb,pdg-a4001n-a-000-1a1-ax|\
adb,pdg-a4101n-a-000-1a1-ae|\
adb,av4202n|\
brcm,bcm963281tan|\
brcm,bcm96328avng|\
brcm,bcm96368mvngr|\
comtrend,ar-5381u|\
comtrend,ar-5387un|\
comtrend,vr-3025u|\
comtrend,vr-3025un|\
comtrend,vr-3026e|\
d-link,dsl-274xb-f1|\
d-link,dsl-2750u-c1|\
d-link,dsl-275xb-d1|\
huawei,echolife-hg622|\
huawei,echolife-hg655b|\
nucom,r5010un-v2|\
sagem,fast-2504n|\
sagem,fast-2704-v2|\
technicolor,tg582n|\
technicolor,tg582n-telecom-italia|\
zyxel,p870hw-51a-v2)
	ucidef_add_switch "switch0" \
		"0:lan:1" "1:lan:2" "2:lan:3" "3:lan:4" "8t@eth0"
	;;
alcatel,rg100a|\
belkin,f5d7633|\
brcm,bcm96348gw|\
brcm,bcm96348gw-10|\
brcm,bcm96348gw-11|\
brcm,bcm96358vw|\
brcm,bcm96358vw2|\
bt,voyager-2500v-bb|\
davolink,dv-201amr|\
d-link,dsl-2650u|\
dynalink,rta1025w|\
netgear,dg834gt-pn|\
pirelli,agpf-s0|\
sagem,fast-2404|\
telsey,magic|\
tp-link,td-w8900gb|\
usrobotics,usr9108)
	ucidef_set_interfaces_lan_wan "eth1" "eth0"
	ucidef_add_switch "switch0" \
		"0:lan:4" "1:lan:3" "2:lan:2" "3:lan:1" "5u@eth1"
	;;
asmax,ar-1004g|\
brcm,bcm96338gw|\
brcm,bcm96338w|\
bt,voyager-2110|\
comtrend,ct-5365|\
comtrend,ct-536plus|\
comtrend,ct-6373|\
d-link,dsl-2640b-b|\
d-link,dsl-2640u|\
dynalink,rta1320|\
netgear,dg834g-v4|\
sagem,fast-2604|\
telsey,cpva642)
	ucidef_add_switch "switch0" \
		"0:lan:4" "1:lan:3" "2:lan:2" "3:lan:1" "5u@eth0"
	;;
brcm,bcm963268bu-p300)
	ucidef_add_switch "switch0" \
		"0:lan" "3:lan" "4:lan" "5:lan" "6:lan" "7:lan" "8t@eth0"
	;;
brcm,bcm96368mvwg)
	ucidef_add_switch "switch0" \
		"1:lan" "2:lan" "4:lan" "5:lan" "8t@eth0"
	;;
bt,home-hub-2-a|\
d-link,dsl-274xb-c2|\
huawei,echolife-hg553|\
huawei,echolife-hg556a-a|\
huawei,echolife-hg556a-b|\
huawei,echolife-hg556a-c)
	ucidef_add_switch "switch0" \
		"0:lan:1" "1:lan:2" "2:lan:3" "3:lan:4" "5t@eth0"
	;;
comtrend,ar-5315u|\
innacomm,w3400v6|\
observa,vh4032n|\
sagem,fast-2704n)
	ucidef_add_switch "switch0" \
		"0:lan:4" "1:lan:3" "2:lan:2" "3:lan:1" "8t@eth0"
	;;
comtrend,vg-8050)
	ucidef_add_switch "switch0" \
		"0:lan:4" "1:lan:3" "2:lan:2" "3:lan:1" "4:wan" "8t@eth0"
	;;
comtrend,vr-3032u)
	ucidef_add_switch "switch0" \
		"0:lan:2" "1:lan:3" "2:lan:4" "3:lan:1" "8t@eth0"
	;;
comtrend,wap-5813n)
	ucidef_add_switch "switch0" \
		"0:lan" "1:lan" "2:lan" "3:lan" "4:wan" "5t@eth0"
	;;
d-link,dva-g3810bn-tl|\
huawei,echolife-hg520v|\
sfr,neufbox-4-foxconn-r1|\
sfr,neufbox-4-sercomm-r0)
	ucidef_set_interfaces_lan_wan "eth1.1" "eth0"
	ucidef_add_switch "switch0" \
		"0:lan:4" "1:lan:3" "2:lan:2" "3:lan:1" "5t@eth1"
	;;
huawei,hg253s-v2)
	ucidef_add_switch "switch0" \
		"1:lan:4" "2:lan:3" "3:lan:2" "4:lan:1" "8t@eth0"
	;;
inteno,vg50)
	ucidef_add_switch "switch0" \
		"0:lan" "1:lan" "2:lan" "3:lan" "4:wan" "8t@eth0"
	;;
inventel,livebox-1|\
telsey,cpva502plus)
	ucidef_set_interfaces_lan_wan "eth0" "eth1"
	;;
netgear,dgnd3700-v1)
	ucidef_add_switch "switch0" \
		"1:lan:4" "2:lan:3" "3:lan:2" "4:lan:1" "0:wan" "8t@eth0"
	;;
sercomm,ad1018|\
sercomm,ad1018-nor)
	ucidef_add_switch "switch0" \
		"1:lan:3" "2:lan:2" "3:lan:1" "0:wan" "8t@eth0"
	;;
sercomm,h500-s-lowi|\
sercomm,h500-s-vfes)
	ucidef_add_switch "switch0" "4:lan" "3:wan" "8t@eth0"
	;;
sfr,neufbox-6-sercomm-r0)
	ucidef_add_switch "switch0" \
		"1:lan" "2:lan" "3:lan" "4:lan" "0:wan" "9t@eth0"
	;;
sky,sr102)
	ucidef_set_interfaces_lan_wan "eth0.1" "eth0.2"
	ucidef_add_switch "switch0" \
		"0:lan" "1:lan" "2:lan" "3:wan" "8t@eth0"
	;;
*)
	ucidef_set_interfaces_lan_wan "eth1" "eth0"
	;;
esac

board_config_flush

exit 0
