From 2a0e0c15c001bfde3666f159552e414217fe44ac Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.org>
Date: Thu, 9 Feb 2017 14:36:44 +0000
Subject: [PATCH] sound: Demote deferral errors to INFO level

At present there is no mechanism to specify driver load order,
which can lead to deferrals and repeated retries until successful.
Since this situation is expected, reduce the dmesg level to
INFO and mention that the operation will be retried.

Signed-off-by: Phil Elwell <phil@raspberrypi.org>
---
 sound/soc/soc-core.c | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

--- a/sound/soc/soc-core.c
+++ b/sound/soc/soc-core.c
@@ -1016,7 +1016,7 @@ int snd_soc_add_pcm_runtime(struct snd_s
 	for_each_link_cpus(dai_link, i, cpu) {
 		asoc_rtd_to_cpu(rtd, i) = snd_soc_find_dai(cpu);
 		if (!asoc_rtd_to_cpu(rtd, i)) {
-			dev_info(card->dev, "ASoC: CPU DAI %s not registered\n",
+			dev_info(card->dev, "ASoC: CPU DAI %s not registered - will retry\n",
 				 cpu->dai_name);
 			goto _err_defer;
 		}
@@ -1027,7 +1027,7 @@ int snd_soc_add_pcm_runtime(struct snd_s
 	for_each_link_codecs(dai_link, i, codec) {
 		asoc_rtd_to_codec(rtd, i) = snd_soc_find_dai(codec);
 		if (!asoc_rtd_to_codec(rtd, i)) {
-			dev_info(card->dev, "ASoC: CODEC DAI %s not registered\n",
+			dev_info(card->dev, "ASoC: CODEC DAI %s not registered- will retry\n",
 				 codec->dai_name);
 			goto _err_defer;
 		}
