// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "ar7100.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	aliases {
		led-boot = &led_rf;
		led-failsafe = &led_rf;
		led-running = &led_rf;
		led-upgrade = &led_rf;
	};

	extosc: ref {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-output-names = "ref";
		clock-frequency = <40000000>;
	};

	leds {
		compatible = "gpio-leds";

		led_rf: rf_green {
			label = "green:rf";
			gpios = <&gpio 2 GPIO_ACTIVE_HIGH>;
		};
	};

	keys {
		compatible = "gpio-keys";

		wps {
			label = "sw4";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 8 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};
	};
};

&eth0 {
	status = "okay";
};

&eth1 {
	status = "okay";
};

&pcie0 {
	status = "okay";
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "ecoscentric,redboot-fis-partitions";
		};
	};
};

&usb_phy {
	status = "okay";
};

&usb1 {
	status = "okay";
	#address-cells = <1>;
	#size-cells = <0>;

	usb_ohci_port: port@1 {
		reg = <1>;
		#trigger-source-cells = <0>;
	};
};

&usb2 {
	status = "okay";
	#address-cells = <1>;
	#size-cells = <0>;

	usb_ehci_port: port@1 {
		reg = <1>;
		#trigger-source-cells = <0>;
	};
};
