From 5b95bb7b2d6b1a866c3ddd752bdbcfa09b0657b0 Mon Sep 17 00:00:00 2001
From: Dave Stevenson <dave.stevenson@raspberrypi.com>
Date: Thu, 11 Jun 2020 13:41:43 +0100
Subject: [PATCH] media: i2c: imx290: Correct range for V4L2_CID_GAIN
 to 0-238

The datasheet lists the gain as being 0.0 to 72.0dB in 0.3dB steps, which
makes 238 steps total.
Correct the 0-72 range defined in the driver.

Signed-off-by: Dave Stevenson <dave.stevenson@raspberrypi.com>
---
 drivers/media/i2c/imx290.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/media/i2c/imx290.c
+++ b/drivers/media/i2c/imx290.c
@@ -1124,7 +1124,7 @@ static int imx290_probe(struct i2c_clien
 	v4l2_ctrl_handler_init(&imx290->ctrls, 4);
 
 	v4l2_ctrl_new_std(&imx290->ctrls, &imx290_ctrl_ops,
-			  V4L2_CID_GAIN, 0, 72, 1, 0);
+			  V4L2_CID_GAIN, 0, 238, 1, 0);
 
 	imx290->link_freq =
 		v4l2_ctrl_new_int_menu(&imx290->ctrls, &imx290_ctrl_ops,
