// SPDX-License-Identifier: GPL-2.0-or-later

#include "mt7621.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

/ {
	compatible = "tplink,eap235-wall-v1", "mediatek,mt7621-soc";
	model = "TP-Link EAP235-Wall v1";

	aliases {
		label-mac-device = &gmac0;
		led-boot = &led_status;
		led-failsafe = &led_status;
		led-running = &led_status;
		led-upgrade = &led_status;
	};

	leds {
		compatible = "gpio-leds";

		led_status: status {
			label = "white:status";
			color = <LED_COLOR_ID_WHITE>;
			function = LED_FUNCTION_STATUS;
			gpios = <&gpio 12 GPIO_ACTIVE_LOW>;
		};
	};

	keys {
		compatible = "gpio-keys";

		led {
			label = "led";
			gpios = <&gpio 10 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_LIGHTS_TOGGLE>;
		};

		reset {
			label = "reset";
			gpios = <&gpio 8 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};

	gpio-export {
		compatible = "gpio-export";

		poe_passthrough {
			gpio-export,name = "poe-passthrough";
			gpio-export,output = <0>;
			gpios = <&gpio 7 GPIO_ACTIVE_HIGH>;
		};
	};
};

&spi0 {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <20000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x00000 0x80000>;
				read-only;
			};

			partition@80000 {
				label = "partition-table";
				reg = <0x80000 0x10000>;
				read-only;
			};

			info: partition@90000 {
				label = "product-info";
				reg = <0x90000 0x10000>;
				read-only;
			};

			partition@a0000 {
				compatible = "tplink,firmware";
				label = "firmware";
				reg = <0x0a0000 0xd20000>;
			};

			partition@dc0000 {
				label = "user-config";
				reg = <0xdc0000 0x030000>;
				read-only;
			};

			/* 0xdf0000 - 0xf30000 unused  */

			partition@f30000 {
				label = "mutil-log";
				reg = <0xf30000 0x080000>;
				read-only;
			};

			partition@fb0000 {
				label = "oops";
				reg = <0xfb0000 0x040000>;
				read-only;
			};

			radio: partition@ff0000 {
				label = "radio";
				reg = <0xff0000 0x010000>;
				read-only;
			};
		};
	};
};

&state_default {
	gpio {
		groups = "uart2", "uart3";
		function = "gpio";
	};
};

&pcie {
	status = "okay";
};

&pcie0 {
	wifi@0,0 {
		reg = <0x0000 0 0 0 0>;
		mediatek,mtd-eeprom = <&radio 0x0>;
		nvmem-cells = <&macaddr_info_8>;
		nvmem-cell-names = "mac-address";
	};
};

&pcie1 {
	wifi@0,0 {
		reg = <0x0000 0 0 0 0>;
		mediatek,mtd-eeprom = <&radio 0x8000>;
		ieee80211-freq-limit = <5000000 6000000>;
		nvmem-cells = <&macaddr_info_8>;
		nvmem-cell-names = "mac-address";
		mac-address-increment = <1>;
	};
};

&gmac0 {
	nvmem-cells = <&macaddr_info_8>;
	nvmem-cell-names = "mac-address";
};

&switch0 {
	ports {
		port@0 {
			status = "okay";
			label = "lan0";
		};

		port@1 {
			status = "okay";
			label = "lan3";
		};

		port@2 {
			status = "okay";
			label = "lan2";
		};

		port@3 {
			status = "okay";
			label = "lan1";
		};
	};
};

&info {
	compatible = "nvmem-cells";
	#address-cells = <1>;
	#size-cells = <1>;

	macaddr_info_8: macaddr@8 {
		reg = <0x8 0x6>;
	};
};
