/dts-v1/;

/ {
	#address-cells = <1>;
	#size-cells = <1>;
	compatible = "brcm,bcm6362";

	aliases {
		nflash = &nflash;
		pinctrl = &pinctrl;
		serial0 = &uart0;
		serial1 = &uart1;
		spi0 = &lsspi;
		spi1 = &hsspi;
	};

	cpus {
		#address-cells = <1>;
		#size-cells = <0>;

		cpu@0 {
			compatible = "brcm,bmips4350", "mips,mips4Kc";
			device_type = "cpu";
			reg = <0>;
		};

		cpu@1 {
			compatible = "brcm,bmips4350", "mips,mips4Kc";
			device_type = "cpu";
			reg = <1>;
		};
	};

	cpu_intc: interrupt-controller {
		#address-cells = <0>;
		compatible = "mti,cpu-interrupt-controller";

		interrupt-controller;
		#interrupt-cells = <1>;
	};

	memory { device_type = "memory"; reg = <0 0>; };

	ubus@10000000 {
		#address-cells = <1>;
		#size-cells = <1>;
		ranges;
		compatible = "simple-bus";
		interrupt-parent = <&periph_intc>;

		ext_intc: interrupt-controller@10000018 {
			compatible = "brcm,bcm6345-ext-intc";
			reg = <0x10000018 0x4>;

			interrupt-controller;
			#interrupt-cells = <2>;

			interrupts = <40>, <41>, <42>, <43>;
		};

		periph_intc: interrupt-controller@10000020 {
			compatible = "brcm,bcm6345-l1-intc";
			reg = <0x10000020 0x10>,
			      <0x10000030 0x10>;

			interrupt-controller;
			#interrupt-cells = <1>;

			interrupt-parent = <&cpu_intc>;
			interrupts = <2>, <3>;
		};

		pinctrl: pin-controller@10000080 {
			compatible = "brcm,bcm6362-pinctrl";
			reg = <0x10000080 0x8>,
			      <0x10000088 0x8>,
			      <0x10000090 0x4>,
			      <0x10000098 0x4>,
			      <0x1000009c 0x4>,
			      <0x100000b8 0x4>;
			reg-names = "dirout", "dat", "led",
				    "mode", "ctrl", "basemode";

			gpio-controller;
			#gpio-cells = <2>;

			interrupt-parent = <&ext_intc>;
			interrupts = <0 0>, <1 0>, <2 0>, <3 0>;
			interrupt-names = "gpio24", "gpio25",
					  "gpio26", "gpio27";

			pinctrl_usb_device_led: usb_device_led {
				function = "usb_device_led";
				pins = "gpio0";
			};

			pinctrl_sys_irq: sys_irq {
				function = "sys_irq";
				pins = "gpio1";
			};

			pinctrl_serial_led: serial_led {
				pinctrl_serial_led_clk: serial_led_clk {
					function = "serial_led_clk";
					pins = "gpio2";
				};

				pinctrl_serial_led_data: serial_led_data {
					function = "serial_led_data";
					pins = "gpio3";
				};
			};

			pinctrl_robosw_led_data: robosw_led_data {
				function = "robosw_led_data";
				pins = "gpio4";
			};

			pinctrl_robosw_led_clk: robosw_led_clk {
				function = "robosw_led_clk";
				pins = "gpio5";
			};

			pinctrl_robosw_led0: robosw_led0 {
				function = "robosw_led0";
				pins = "gpio6";
			};

			pinctrl_robosw_led1: robosw_led1 {
				function = "robosw_led1";
				pins = "gpio7";
			};

			pinctrl_inet_led: inet_led {
				function = "inet_led";
				pins = "gpio8";
			};

			pinctrl_spi_cs2: spi_cs2 {
				function = "spi_cs2";
				pins = "gpio9";
			};

			pinctrl_spi_cs3: spi_cs3 {
				function = "spi_cs3";
				pins = "gpio10";
			};

			pinctrl_ntr_pulse: ntr_pulse {
				function = "ntr_pulse";
				pins = "gpio11";
			};

			pinctrl_uart1_scts: uart1_scts {
				function = "uart1_scts";
				pins = "gpio12";
			};

			pinctrl_uart1_srts: uart1_srts {
				function = "uart1_srts";
				pins = "gpio13";
			};


			pinctrl_uart1: uart1 {
				pinctrl_uart1_sdin: uart1_sdin {
					function = "uart1_sdin";
					pins = "gpio14";
				};

				pinctrl_uart1_sdout: uart1_sdout {
					function = "uart1_sdout";
					pins = "gpio15";
				};
			};

			pinctrl_adsl_spi: adsl_spi {
				pinctrl_adsl_spi_miso: adsl_spi_miso {
					function = "adsl_spi_miso";
					pins = "gpio16";
				};

				pinctrl_adsl_spi_mosi: adsl_spi_mosi {
					function = "adsl_spi_mosi";
					pins = "gpio17";
				};

				pinctrl_adsl_spi_clk: adsl_spi_clk {
					function = "adsl_spi_clk";
					pins = "gpio18";
				};

				pinctrl_adsl_spi_cs: adsl_spi_cs {
					function = "adsl_spi_cs";
					pins = "gpio19";
				};
			};

			pinctrl_ephy0_led: ephy0_led {
				function = "ephy0_led";
				pins = "gpio20";
			};

			pinctrl_ephy1_led: ephy1_led {
				function = "ephy1_led";
				pins = "gpio21";
			};

			pinctrl_ephy2_led: ephy2_led {
				function = "ephy2_led";
				pins = "gpio22";
			};

			pinctrl_ephy3_led: ephy3_led {
				function = "ephy3_led";
				pins = "gpio23";
			};

			pinctrl_ext_irq0: ext_irq0 {
				function = "ext_irq0";
				pins = "gpio24";
			};

			pinctrl_ext_irq1: ext_irq1 {
				function = "ext_irq1";
				pins = "gpio25";
			};

			pinctrl_ext_irq2: ext_irq2 {
				function = "ext_irq2";
				pins = "gpio26";
			};

			pinctrl_ext_irq3: ext_irq3 {
				function = "ext_irq3";
				pins = "gpio27";
			};

			pinctrl_nand: nand {
				function = "nand";
				group = "nand_grp";
			};
		};

		uart0: serial@10000100 {
			compatible = "brcm,bcm6345-uart";
			reg = <0x10000100 0x18>;

			interrupt-parent = <&periph_intc>;
			interrupts = <3>;

			/* clocks = <&periph_clk>; */
			/* clock-names = "refclk"; */

			status = "disabled";
		};

		uart1: serial@10000120 {
			compatible = "brcm,bcm6345-uart";
			reg = <0x10000120 0x18>;

			interrupt-parent = <&periph_intc>;
			interrupts = <4>;

			/* clocks = <&periph_clk>; */
			/* clock-names = "refclk"; */

			status = "disabled";
		};

		lsspi: spi@10000800 {
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "brcm,bcm6358-spi";
			reg = <0x10000800 0x70c>;
			interrupts = <2>;
			/* clocks = <&clkctl 15>; */
		};

		hsspi: spi@10001000 {
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "brcm,bcm6328-hsspi";
			reg = <0x10001000 0x600>;
			interrupts = <5>;
			/* clocks = <&clkctl 16>; */
		};

		nflash: nand@10000200 {
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "brcm,nand-bcm6368",
				     "brcm,brcmnand-v2.2",
				     "brcm,brcmnand";
			reg = <0x10000200 0x180>,
			      <0x10000600 0x200>,
			      <0x10000070 0x10>;
			reg-names = "nand",
				    "nand-cache",
				    "nand-int-base";

			interrupt-parent = <&periph_intc>;
			interrupts = <12>;

			/* clocks = <&clkctl 20>; */

			pinctrl-names = "default";
			pinctrl-0 = <&pinctrl_nand>;

			status = "disabled";
		};

		leds: led-controller@10001900 {
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "brcm,bcm6328-leds";
			reg = <0x10001900 0x24>;
			status = "disabled";
		};
	};
};
