From b6eaf8158d0e2053680dc72e45d2a4e7d0617312 Mon Sep 17 00:00:00 2001
From: Dave Stevenson <dave.stevenson@raspberrypi.com>
Date: Tue, 7 Jul 2020 11:51:26 +0100
Subject: [PATCH] media: i2c: imx290: Set the colorspace fields in the
 format

The colorspace fields were left untouched in imx290_set_fmt
which lead to a v4l2-compliance failure.

Signed-off-by: Dave Stevenson <dave.stevenson@raspberrypi.com>
---
 drivers/media/i2c/imx290.c | 8 ++++++++
 1 file changed, 8 insertions(+)

--- a/drivers/media/i2c/imx290.c
+++ b/drivers/media/i2c/imx290.c
@@ -813,6 +813,14 @@ static int imx290_set_fmt(struct v4l2_su
 
 	fmt->format.code = imx290->formats[i].code;
 	fmt->format.field = V4L2_FIELD_NONE;
+	fmt->format.colorspace = V4L2_COLORSPACE_SRGB;
+	fmt->format.ycbcr_enc =
+			V4L2_MAP_YCBCR_ENC_DEFAULT(fmt->format.colorspace);
+	fmt->format.quantization =
+		V4L2_MAP_QUANTIZATION_DEFAULT(true, fmt->format.colorspace,
+					      fmt->format.ycbcr_enc);
+	fmt->format.xfer_func =
+		V4L2_MAP_XFER_FUNC_DEFAULT(fmt->format.colorspace);
 
 	if (fmt->which == V4L2_SUBDEV_FORMAT_TRY) {
 		format = v4l2_subdev_get_try_format(sd, cfg, fmt->pad);
