#include "bcm63268.dtsi"

#include <dt-bindings/input/input.h>

/ {
	model = "SKY SR102";
	compatible = "sky,sr102", "brcm,bcm63168", "brcm,bcm63268";

	aliases {
		led-boot = &led_power_white;
		led-failsafe = &led_power_white;
		led-running = &led_power_white;
		led-upgrade = &led_power_white;
	};

	chosen {
		bootargs = "rootfstype=squashfs,jffs2 noinitrd console=ttyS0,115200";
		stdout-path = "serial0:115200n8";
	};

	keys {
		compatible = "gpio-keys-polled";
		#address-cells = <1>;
		#size-cells = <0>;
		poll-interval = <20>;

		wps {
			label = "wps";
			gpios = <&pinctrl 33 0>;
			linux,code = <KEY_WPS_BUTTON>;
			debounce-interval = <60>;
		};
	};

	leds {
		compatible = "gpio-leds";

		lan1_green {
			label = "green:lan1";
			gpios = <&pinctrl 1 1>;
		};
		power_red {
			label = "red:power";
			gpios = <&pinctrl 2 1>;
		};
		wifi_red {
			label = "red:wifi";
			gpios = <&pinctrl 3 1>;
		};
		inet_red {
			label = "red:inet";
			gpios = <&pinctrl 4 1>;
		};
		inet_white {
			label = "white:inet";
			gpios = <&pinctrl 5 0>;
		};
		led_power_white: power_white {
			label = "white:power";
			gpios = <&pinctrl 6 0>;
			default-state = "on";
		};
		wifi_white {
			label = "white:wifi";
			gpios = <&pinctrl 8 0>;
		};
		lan2_red {
			label = "red:lan2";
			gpios = <&pinctrl 9 1>;
		};
		lan3_red {
			label = "red:lan3";
			gpios = <&pinctrl 10 1>;
		};
		lan4_red {
			label = "red:lan4";
			gpios = <&pinctrl 11 1>;
		};
		lan1_red {
			label = "red:lan1";
			gpios = <&pinctrl 12 1>;
		};
		lan2_green {
			label = "green:lan2";
			gpios = <&pinctrl 13 0>;
		};
		lan3_green {
			label = "green:lan3";
			gpios = <&pinctrl 14 1>;
		};
		lan4_green {
			label = "green:lan4";
			gpios = <&pinctrl 15 1>;
		};
		hd_white {
			label = "white:hd";
			gpios = <&pinctrl 18 0>;
		};
	};
};

&hsspi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		spi-max-frequency = <16666667>;
		spi-tx-bus-width = <2>;
		spi-rx-bus-width = <2>;
		reg = <0>;

		#address-cells = <1>;
		#size-cells = <1>;

		partitions {
			compatible = "brcm,bcm963xx-cfe-nor-partitions";
		};
	};
};

&uart0 {
	status = "okay";
};
