#include "bcm6358.dtsi"

#include <dt-bindings/input/input.h>

/ {
	model = "Huawei EchoLife HG553";
	compatible = "huawei,echolife-hg553", "brcm,bcm6358";

	aliases {
		led-boot = &led_power_blue;
		led-failsafe = &led_power_blue;
		led-running = &led_power_blue;
		led-upgrade = &led_power_blue;
	};

	chosen {
		bootargs = "rootfstype=squashfs,jffs2 noinitrd console=ttyS0,115200";
		stdout-path = "serial0:115200n8";
	};

	keys {
		compatible = "gpio-keys-polled";
		#address-cells = <1>;
		#size-cells = <0>;
		poll-interval = <20>;

		rfkill {
			label = "rfkill";
			gpios = <&pinctrl 9 1>;
			linux,code = <KEY_RFKILL>;
			debounce-interval = <60>;
		};

		reset {
			label = "reset";
			gpios = <&pinctrl 37 1>;
			linux,code = <KEY_RESTART>;
			debounce-interval = <60>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_power_blue: power_blue {
			label = "blue:power";
			gpios = <&pinctrl 4 1>;
			default-state = "on";
		};
		power_red {
			label = "red:power";
			gpios = <&pinctrl 5 1>;
		};
		hspa_red {
			label = "red:hspa";
			gpios = <&pinctrl 12 1>;
		};
		hspa_blue {
			label = "blue:hspa";
			gpios = <&pinctrl 13 1>;
		};
		lan_red {
			label = "red:lan";
			gpios = <&pinctrl 22 1>;
		};
		lan_blue {
			label = "blue:lan";
			gpios = <&pinctrl 23 1>;
		};
		wifi_red {
			label = "red:wifi";
			gpios = <&pinctrl 25 1>;
		};
		dsl_red {
			label = "red:adsl";
			gpios = <&pinctrl 34 1>;
		};
		dsl_blue {
			label = "blue:adsl";
			gpios = <&pinctrl 35 1>;
		};
	};
};

&pflash {
	status = "okay";

	partitions {
		compatible = "fixed-partitions";
		#address-cells = <1>;
		#size-cells = <1>;

		cfe@0 {
			label = "CFE";
			reg = <0x000000 0x020000>;
			read-only;
		};

		linux@20000 {
			label = "linux";
			reg = <0x020000 0xfc0000>;
			compatible = "brcm,bcm963xx-imagetag";
		};

		nvram@fe0000 {
			label = "nvram";
			reg = <0xfe0000 0x020000>;
		};
	};
};

&uart0 {
	status = "okay";
};
