From 636a1e697555e73c28cdd6952a409edbfdd16475 Mon Sep 17 00:00:00 2001
From: Chris Blake <chrisrblake93@gmail.com>
Date: Mon, 9 Aug 2021 19:40:21 -0500
Subject: platform/x86: add meraki-mx100 platform driver

This adds platform support for the Cisco Meraki MX100 (Tinkerbell)
network appliance. This sets up the network LEDs and Reset
button.

Depends-on: ef0eea5b151ae ("mfd: lpc_ich: Enable GPIO driver for DH89xxCC")
Co-developed-by: Christian Lamparter <chunkeey@gmail.com>
Signed-off-by: Christian Lamparter <chunkeey@gmail.com>
Signed-off-by: Chris Blake <chrisrblake93@gmail.com>
Reviewed-by: Andy Shevchenko <andy.shevchenko@gmail.com>
Link: https://lore.kernel.org/r/20210810004021.2538308-1-chrisrblake93@gmail.com
Reviewed-by: Hans de Goede <hdegoede@redhat.com>
Signed-off-by: Hans de Goede <hdegoede@redhat.com>
---
 drivers/platform/x86/Kconfig        |  13 ++
 drivers/platform/x86/Makefile       |   3 +
 drivers/platform/x86/meraki-mx100.c | 230 ++++++++++++++++++++++++++++++++++++
 3 files changed, 246 insertions(+)
 create mode 100644 drivers/platform/x86/meraki-mx100.c

diff --git a/drivers/platform/x86/Kconfig b/drivers/platform/x86/Kconfig
index 6ad35158ae4ef..432d72170b003 100644
--- a/drivers/platform/x86/Kconfig
+++ b/drivers/platform/x86/Kconfig
@@ -302,6 +302,19 @@ config ASUS_NB_WMI
 	  If you have an ACPI-WMI compatible Asus Notebook, say Y or M
 	  here.
 
+config MERAKI_MX100
+	tristate "Cisco Meraki MX100 Platform Driver"
+	depends on GPIOLIB
+	depends on GPIO_ICH
+	depends on LEDS_CLASS
+	select LEDS_GPIO
+	help
+	  This driver provides support for the front button and LEDs on
+	  the Cisco Meraki MX100 (Tinkerbell) 1U appliance.
+
+	  To compile this driver as a module, choose M here: the module
+	  will be called meraki-mx100.
+
 config EEEPC_LAPTOP
 	tristate "Eee PC Hotkey Driver"
 	depends on ACPI
diff --git a/drivers/platform/x86/Makefile b/drivers/platform/x86/Makefile
index 5edfdc2ea7f29..9bb3c3f773864 100644
--- a/drivers/platform/x86/Makefile
+++ b/drivers/platform/x86/Makefile
@@ -39,6 +39,9 @@ obj-$(CONFIG_ASUS_NB_WMI)	+= asus-nb-wmi.o
 obj-$(CONFIG_EEEPC_LAPTOP)	+= eeepc-laptop.o
 obj-$(CONFIG_EEEPC_WMI)		+= eeepc-wmi.o
 
+# Cisco/Meraki
+obj-$(CONFIG_MERAKI_MX100)	+= meraki-mx100.o
+
 # Dell
 obj-$(CONFIG_X86_PLATFORM_DRIVERS_DELL)		+= dell/
 
diff --git a/drivers/platform/x86/meraki-mx100.c b/drivers/platform/x86/meraki-mx100.c
new file mode 100644
index 0000000000000..3751ed36a980a
--- /dev/null
+++ b/drivers/platform/x86/meraki-mx100.c
@@ -0,0 +1,230 @@
+// SPDX-License-Identifier: GPL-2.0+
+
+/*
+ * Cisco Meraki MX100 (Tinkerbell) board platform driver
+ *
+ * Based off of arch/x86/platform/meraki/tink.c from the
+ * Meraki GPL release meraki-firmware-sources-r23-20150601
+ *
+ * Format inspired by platform/x86/pcengines-apuv2.c
+ *
+ * Copyright (C) 2021 Chris Blake <chrisrblake93@gmail.com>
+ */
+
+#define pr_fmt(fmt)	KBUILD_MODNAME ": " fmt
+
+#include <linux/dmi.h>
+#include <linux/err.h>
+#include <linux/gpio_keys.h>
+#include <linux/gpio/machine.h>
+#include <linux/input.h>
+#include <linux/io.h>
+#include <linux/kernel.h>
+#include <linux/leds.h>
+#include <linux/module.h>
+#include <linux/platform_device.h>
+
+#define TINK_GPIO_DRIVER_NAME "gpio_ich"
+
+/* LEDs */
+static const struct gpio_led tink_leds[] = {
+	{
+		.name = "mx100:green:internet",
+		.default_trigger = "default-on",
+	},
+	{
+		.name = "mx100:green:lan2",
+	},
+	{
+		.name = "mx100:green:lan3",
+	},
+	{
+		.name = "mx100:green:lan4",
+	},
+	{
+		.name = "mx100:green:lan5",
+	},
+	{
+		.name = "mx100:green:lan6",
+	},
+	{
+		.name = "mx100:green:lan7",
+	},
+	{
+		.name = "mx100:green:lan8",
+	},
+	{
+		.name = "mx100:green:lan9",
+	},
+	{
+		.name = "mx100:green:lan10",
+	},
+	{
+		.name = "mx100:green:lan11",
+	},
+	{
+		.name = "mx100:green:ha",
+	},
+	{
+		.name = "mx100:orange:ha",
+	},
+	{
+		.name = "mx100:green:usb",
+	},
+	{
+		.name = "mx100:orange:usb",
+	},
+};
+
+static const struct gpio_led_platform_data tink_leds_pdata = {
+	.num_leds	= ARRAY_SIZE(tink_leds),
+	.leds		= tink_leds,
+};
+
+static struct gpiod_lookup_table tink_leds_table = {
+	.dev_id = "leds-gpio",
+	.table = {
+		GPIO_LOOKUP_IDX(TINK_GPIO_DRIVER_NAME, 11,
+				NULL, 0, GPIO_ACTIVE_LOW),
+		GPIO_LOOKUP_IDX(TINK_GPIO_DRIVER_NAME, 18,
+				NULL, 1, GPIO_ACTIVE_HIGH),
+		GPIO_LOOKUP_IDX(TINK_GPIO_DRIVER_NAME, 20,
+				NULL, 2, GPIO_ACTIVE_HIGH),
+		GPIO_LOOKUP_IDX(TINK_GPIO_DRIVER_NAME, 22,
+				NULL, 3, GPIO_ACTIVE_HIGH),
+		GPIO_LOOKUP_IDX(TINK_GPIO_DRIVER_NAME, 23,
+				NULL, 4, GPIO_ACTIVE_HIGH),
+		GPIO_LOOKUP_IDX(TINK_GPIO_DRIVER_NAME, 32,
+				NULL, 5, GPIO_ACTIVE_HIGH),
+		GPIO_LOOKUP_IDX(TINK_GPIO_DRIVER_NAME, 34,
+				NULL, 6, GPIO_ACTIVE_HIGH),
+		GPIO_LOOKUP_IDX(TINK_GPIO_DRIVER_NAME, 35,
+				NULL, 7, GPIO_ACTIVE_HIGH),
+		GPIO_LOOKUP_IDX(TINK_GPIO_DRIVER_NAME, 36,
+				NULL, 8, GPIO_ACTIVE_HIGH),
+		GPIO_LOOKUP_IDX(TINK_GPIO_DRIVER_NAME, 37,
+				NULL, 9, GPIO_ACTIVE_HIGH),
+		GPIO_LOOKUP_IDX(TINK_GPIO_DRIVER_NAME, 48,
+				NULL, 10, GPIO_ACTIVE_HIGH),
+		GPIO_LOOKUP_IDX(TINK_GPIO_DRIVER_NAME, 16,
+				NULL, 11, GPIO_ACTIVE_LOW),
+		GPIO_LOOKUP_IDX(TINK_GPIO_DRIVER_NAME, 7,
+				NULL, 12, GPIO_ACTIVE_LOW),
+		GPIO_LOOKUP_IDX(TINK_GPIO_DRIVER_NAME, 21,
+				NULL, 13, GPIO_ACTIVE_LOW),
+		GPIO_LOOKUP_IDX(TINK_GPIO_DRIVER_NAME, 19,
+				NULL, 14, GPIO_ACTIVE_LOW),
+		{} /* Terminating entry */
+	}
+};
+
+/* Reset Button */
+static struct gpio_keys_button tink_buttons[] = {
+	{
+		.desc			= "Reset",
+		.type			= EV_KEY,
+		.code			= KEY_RESTART,
+		.active_low             = 1,
+		.debounce_interval      = 100,
+	},
+};
+
+static const struct gpio_keys_platform_data tink_buttons_pdata = {
+	.buttons	= tink_buttons,
+	.nbuttons	= ARRAY_SIZE(tink_buttons),
+	.poll_interval  = 20,
+	.rep		= 0,
+	.name		= "mx100-keys",
+};
+
+static struct gpiod_lookup_table tink_keys_table = {
+	.dev_id = "gpio-keys-polled",
+	.table = {
+		GPIO_LOOKUP_IDX(TINK_GPIO_DRIVER_NAME, 60,
+				NULL, 0, GPIO_ACTIVE_LOW),
+		{} /* Terminating entry */
+	}
+};
+
+/* Board setup */
+static const struct dmi_system_id tink_systems[] __initconst = {
+	{
+		.matches = {
+			DMI_EXACT_MATCH(DMI_SYS_VENDOR, "Cisco"),
+			DMI_EXACT_MATCH(DMI_PRODUCT_NAME, "MX100-HW"),
+		},
+	},
+	{} /* Terminating entry */
+};
+MODULE_DEVICE_TABLE(dmi, tink_systems);
+
+static struct platform_device *tink_leds_pdev;
+static struct platform_device *tink_keys_pdev;
+
+static struct platform_device * __init tink_create_dev(
+	const char *name, const void *pdata, size_t sz)
+{
+	struct platform_device *pdev;
+
+	pdev = platform_device_register_data(NULL,
+		name, PLATFORM_DEVID_NONE, pdata, sz);
+	if (IS_ERR(pdev))
+		pr_err("failed registering %s: %ld\n", name, PTR_ERR(pdev));
+
+	return pdev;
+}
+
+static int __init tink_board_init(void)
+{
+	int ret;
+
+	if (!dmi_first_match(tink_systems))
+		return -ENODEV;
+
+	/*
+	 * We need to make sure that GPIO60 isn't set to native mode as is default since it's our
+	 * Reset Button. To do this, write to GPIO_USE_SEL2 to have GPIO60 set to GPIO mode.
+	 * This is documented on page 1609 of the PCH datasheet, order number 327879-005US
+	 */
+	outl(inl(0x530) | BIT(28), 0x530);
+
+	gpiod_add_lookup_table(&tink_leds_table);
+	gpiod_add_lookup_table(&tink_keys_table);
+
+	tink_leds_pdev = tink_create_dev("leds-gpio",
+		&tink_leds_pdata, sizeof(tink_leds_pdata));
+	if (IS_ERR(tink_leds_pdev)) {
+		ret = PTR_ERR(tink_leds_pdev);
+		goto err;
+	}
+
+	tink_keys_pdev = tink_create_dev("gpio-keys-polled",
+		&tink_buttons_pdata, sizeof(tink_buttons_pdata));
+	if (IS_ERR(tink_keys_pdev)) {
+		ret = PTR_ERR(tink_keys_pdev);
+		platform_device_unregister(tink_leds_pdev);
+		goto err;
+	}
+
+	return 0;
+
+err:
+	gpiod_remove_lookup_table(&tink_keys_table);
+	gpiod_remove_lookup_table(&tink_leds_table);
+	return ret;
+}
+module_init(tink_board_init);
+
+static void __exit tink_board_exit(void)
+{
+	platform_device_unregister(tink_keys_pdev);
+	platform_device_unregister(tink_leds_pdev);
+	gpiod_remove_lookup_table(&tink_keys_table);
+	gpiod_remove_lookup_table(&tink_leds_table);
+}
+module_exit(tink_board_exit);
+
+MODULE_AUTHOR("Chris Blake <chrisrblake93@gmail.com>");
+MODULE_DESCRIPTION("Cisco Meraki MX100 Platform Driver");
+MODULE_LICENSE("GPL");
+MODULE_ALIAS("platform:meraki-mx100");
-- 
cgit 1.2.3-1.el7
