From 3a5f1793c0bf4a6b536751886b0a44589fe05f35 Mon Sep 17 00:00:00 2001
From: Ansuel Smith <ansuelsmth@gmail.com>
Date: Sun, 7 Feb 2021 17:00:07 +0100
Subject: [PATCH 2/4] ipq806x: lcc: add missing reset

Add missing reset for ipq806x lcc clk

Signed-off-by: Ansuel Smith <ansuelsmth@gmail.com>
---
 drivers/clk/qcom/lcc-ipq806x.c               | 8 ++++++++
 include/dt-bindings/clock/qcom,lcc-ipq806x.h | 1 +
 2 files changed, 9 insertions(+)

--- a/drivers/clk/qcom/lcc-ipq806x.c
+++ b/drivers/clk/qcom/lcc-ipq806x.c
@@ -12,6 +12,7 @@
 #include <linux/of_device.h>
 #include <linux/clk-provider.h>
 #include <linux/regmap.h>
+#include <linux/reset-controller.h>
 
 #include <dt-bindings/clock/qcom,lcc-ipq806x.h>
 
@@ -22,6 +23,7 @@
 #include "clk-branch.h"
 #include "clk-regmap-divider.h"
 #include "clk-regmap-mux.h"
+#include "reset.h"
 
 static struct clk_pll pll4 = {
 	.l_reg = 0x4,
@@ -39,6 +41,10 @@ static struct clk_pll pll4 = {
 	},
 };
 
+static const struct qcom_reset_map lcc_ipq806x_resets[] = {
+	[LCC_PCM_RESET] = { 0x54, 13 },
+};
+
 static const struct pll_config pll4_config = {
 	.l = 0xf,
 	.m = 0x91,
@@ -417,6 +423,8 @@ static const struct qcom_cc_desc lcc_ipq
 	.config = &lcc_ipq806x_regmap_config,
 	.clks = lcc_ipq806x_clks,
 	.num_clks = ARRAY_SIZE(lcc_ipq806x_clks),
+	.resets = lcc_ipq806x_resets,
+	.num_resets = ARRAY_SIZE(lcc_ipq806x_resets),
 };
 
 static const struct of_device_id lcc_ipq806x_match_table[] = {
--- a/include/dt-bindings/clock/qcom,lcc-ipq806x.h
+++ b/include/dt-bindings/clock/qcom,lcc-ipq806x.h
@@ -19,4 +19,5 @@
 #define SPDIF_CLK			10
 #define AHBIX_CLK			11
 
+#define LCC_PCM_RESET			0
 #endif
