// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "qcom-ipq4019.dtsi"
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/soc/qcom,tcsr.h>

/ {
	model = "AVM FRITZ!Repeater 1200";
	compatible = "avm,fritzrepeater-1200";

	aliases {
		led-boot = &power_green;
		led-failsafe = &power_red;
		led-running = &power_green;
		led-upgrade = &power_red;
		label-mac-device = &wifi0;
	};

	soc {
		rng@22000 {
			status = "okay";
		};

		mdio@90000 {
			status = "okay";
			pinctrl-0 = <&mdio_pins>;
			pinctrl-names = "default";

			/delete-node/ ethernet-phy@1;
			/delete-node/ ethernet-phy@2;
			/delete-node/ ethernet-phy@3;
			/delete-node/ ethernet-phy@4;
			/delete-node/ psgmii-phy@5;
		};

		tcsr@1949000 {
			compatible = "qcom,tcsr";
			reg = <0x1949000 0x100>;
			qcom,wifi_glb_cfg = <TCSR_WIFI_GLB_CFG>;
		};

		ess_tcsr@1953000 {
			compatible = "qcom,tcsr";
			reg = <0x1953000 0x1000>;
			qcom,ess-interface-select = <TCSR_ESS_PSGMII_RGMII5>;
		};

		tcsr@1957000 {
			compatible = "qcom,tcsr";
			reg = <0x1957000 0x100>;
			qcom,wifi_noc_memtype_m0_m2 = <TCSR_WIFI_NOC_MEMTYPE_M0_M2>;
		};

		crypto@8e3a000 {
			status = "okay";
		};

		watchdog@b017000 {
			status = "okay";
		};

		ess-switch@c000000 {
			switch_mac_mode = <0x3>; /* mac mode for RGMII RMII */
			switch_lan_bmp = <0x0>; /* lan port bitmap */
			switch_wan_bmp = <0x10>; /* wan port bitmap */
		};

		edma@c080000 {
			status = "okay";
			phy-mode = "rgmii-id";
			qcom,num_gmac = <1>;
			qcom,single-phy;
		};
	};

	key {
		compatible = "gpio-keys";

		wps {
			label = "WPS button";
			gpios = <&tlmm 10 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};
	};

	leds {
		compatible = "gpio-leds";

		power_red: power_red {
			label = "red:power";
			gpios = <&tlmm 50 GPIO_ACTIVE_LOW>;
		};

		power_green: power_green {
			label = "green:power";
			gpios = <&tlmm 45 GPIO_ACTIVE_HIGH>;
		};

		power_yellow {
			label = "yellow:power";
			gpios = <&tlmm 49 GPIO_ACTIVE_LOW>;
		};
	};
};

&tlmm {
	serial_0_pins: serial_pinmux {
		mux {
			pins = "gpio16", "gpio17";
			function = "blsp_uart0";
			bias-disable;
		};
	};

	nand_pins: nand_pins {
		pullups {
			pins = "gpio53", "gpio58", "gpio59";
			function = "qpic";
			bias-pull-up;
		};

		pulldowns {
			pins = "gpio54", "gpio55", "gpio56",
				"gpio57", "gpio60", "gpio61",
				"gpio62", "gpio63", "gpio64",
				"gpio65", "gpio66", "gpio67",
				"gpio68", "gpio69";
			function = "qpic";
			bias-pull-down;
		};
	};

	mdio_pins: mdio_pinmux {
		mux_1 {
			pins = "gpio6";
			function = "mdio";
			bias-pull-up;
		};
		mux_2 {
			pins = "gpio7";
			function = "mdc";
			bias-pull-up;
		};
	};

	phy-reset {
		line-name = "PHY-reset";
		gpios = <19 GPIO_ACTIVE_HIGH>;
		gpio-hog;
		output-high;
	};

	phy-reset-2 {
		line-name = "PHY-reset-2";
		gpios = <47 GPIO_ACTIVE_HIGH>;
		gpio-hog;
		output-high;
	};
};

&nand {
	pinctrl-0 = <&nand_pins>;
	pinctrl-names = "default";
	status = "okay";

	nand@0 {
		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "SBL1";
				reg = <0x0 0x80000>;
				read-only;
			};

			partition@80000 {
				label = "MIBIB";
				reg = <0x80000 0x80000>;
				read-only;
			};

			partition@100000 {
				label = "QSEE";
				reg = <0x100000 0x80000>;
				read-only;
			};

			partition@180000 {
				label = "CDT";
				reg = <0x180000 0x40000>;
				read-only;
			};

			partition@1c0000 {
				label = "QSEE_B";
				reg = <0x1c0000 0x80000>;
				read-only;
			};

			partition@240000 {
				label = "urlader0";
				reg = <0x240000 0x40000>;
				read-only;
			};

			partition@280000 {
				label = "urlader1";
				reg = <0x280000 0x40000>;
				read-only;
			};

			partition@2c0000 {
				label = "nand-tffs";
				reg = <0x2c0000 0x840000>;
				read-only;
			};

			partition@b00000 {
				/* 'kernel1' in AVM firmware */
				label = "uboot0";
				reg = <0xb00000 0x400000>;
			};

			partition@f00000 {
				/* 'kernel2' in AVM firmware */
				label = "uboot1";
				reg = <0xf00000 0x400000>;
			};

			partition@1300000 {
				label = "ubi";
				reg = <0x1300000 0x6d00000>;
			};
		};
	};
};

&cryptobam {
	status = "okay";
};

&blsp_dma {
	status = "okay";
};

&blsp1_uart1 {
	pinctrl-0 = <&serial_0_pins>;
	pinctrl-names = "default";
	status = "okay";
};

&qpic_bam {
	status = "okay";
};

&wifi0 {
	status = "okay";
	qcom,ath10k-calibration-variant = "AVM-FRITZRepeater-1200";
};

&wifi1 {
	status = "okay";
	qcom,ath10k-calibration-variant = "AVM-FRITZRepeater-1200";
};

&gmac0 {
	qcom,phy_mdio_addr = <0>;
	qcom,poll_required = <1>;
	vlan_tag = <0 0x20>;
};
