#include "bcm6328.dtsi"

#include <dt-bindings/input/input.h>

/ {
	model = "Sercomm AD1018 (SPI flash mod)";
	compatible = "sercomm,ad1018-nor", "brcm,bcm6328";

	aliases {
		led-boot = &led_power_green;
		led-failsafe = &led_power_green;
		led-running = &led_power_green;
		led-upgrade = &led_power_green;
	};

	chosen {
		bootargs = "rootfstype=squashfs,jffs2 noinitrd console=ttyS0,115200";
		stdout-path = "serial0:115200n8";
	};

	keys {
		compatible = "gpio-keys-polled";
		#address-cells = <1>;
		#size-cells = <0>;
		poll-interval = <20>;

		wps {
			label = "wps";
			gpios = <&pinctrl 24 1>;
			linux,code = <KEY_WPS_BUTTON>;
			debounce-interval = <60>;
		};

		wifi {
			label = "wifi";
			gpios = <&pinctrl 25 1>;
			linux,code = <KEY_WLAN>;
			debounce-interval = <60>;
		};

		reset {
			label = "reset";
			gpios = <&pinctrl 31 1>;
			linux,code = <KEY_RESTART>;
			debounce-interval = <60>;
		};
	};
};

&pinctrl {
	pinctrl_leds: leds {
		function = "led";
		pins = "gpio0", "gpio1";
	};
};

&leds {
	status = "okay";

	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_leds &pinctrl_serial_led
		     &pinctrl_ephy0_spd_led &pinctrl_ephy1_act_led
		     &pinctrl_ephy2_act_led &pinctrl_ephy3_act_led>;

	brcm,serial-leds;
	brcm,serial-shift-inv;
	brcm,serial-dat-low;

	inet_red@0 {
		reg = <0>;
		active-low;
		label = "red:internet";
	};

	inet_green@1 {
		reg = <1>;
		active-low;
		label = "green:internet";
	};

	led_power_green: power_green@8 {
		reg = <8>;
		active-low;
		label = "green:power";
		default-state = "on";
	};

	adsl_green@10 {
		reg = <10>;
		active-low;
		label = "green:adsl";
	};

	adsl_red@11 {
		reg = <11>;
		active-low;
		label = "red:adsl";
	};

	phone_green@12 {
		reg = <12>;
		active-low;
		label = "green:phone";
	};

	wps_green@13 {
		reg = <13>;
		active-low;
		label = "green:wps";
	};

	wifi_green@14 {
		reg = <14>;
		active-low;
		label = "green:wifi";
	};

	usb_green@15 {
		reg = <15>;
		active-low;
		label = "green:usb";
	};

	ephy0_spd@17 {
		reg = <17>;
		brcm,hardware-controlled;
	};
};

&hsspi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		spi-max-frequency = <16666667>;
		spi-tx-bus-width = <2>;
		spi-rx-bus-width = <2>;
		reg = <0>;

		#address-cells = <1>;
		#size-cells = <1>;

		partitions {
			compatible = "brcm,bcm963xx-cfe-nor-partitions";
		};
	};
};

&nflash {
	status = "okay";

	nandcs@0 {
		compatible = "brcm,nandcs";
		reg = <0>;
		nand-ecc-step-size = <512>;
		nand-ecc-strength = <15>;
		nand-on-flash-bbt;
		brcm,nand-oob-sector-size = <64>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "storage";
				reg = <0 0>; /* autodetected size */
			};
		};
	};
};

&uart0 {
	status = "okay";
};
