// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "ar7242.dtsi"
#include "ar724x_senao_loader-4k.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "engenius,eap350-v1", "qca,ar7242";
	model = "EnGenius EAP350 v1";

	aliases {
		label-mac-device = &eth0;
		led-boot = &led_power;
		led-failsafe = &led_power;
		led-running = &led_power;
		led-upgrade = &led_power;
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			gpios = <&gpio 0 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
			linux,code = <KEY_RESTART>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_power: power {
			label = "blue:power";
			gpios = <&gpio 17 GPIO_ACTIVE_HIGH>;
			default-state = "on";
		};
	};

	ath9k-leds {
		compatible = "gpio-leds";

		wlan {
			label = "blue:wlan";
			gpios = <&ath9k 1 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};
	};
};

&mdio0 {
	status = "okay";

	phy4: ethernet-phy@4 {
		reg = <4>;
		eee-broken-100tx;
		eee-broken-1000t;
	};
};

&eth0 {
	status = "okay";

	nvmem-cells = <&macaddr_art_0>;
	nvmem-cell-names = "mac-address";

	phy-handle = <&phy4>;
	phy-mode = "rgmii-id";

	pll-data = <0x02000000 0x00000101 0x00001313>;
};

&pcie {
	status = "okay";

	ath9k: wifi@0,0,0 {
		compatible = "pci168c,002a";
		reg = <0x0 0 0 0 0>;
		nvmem-cells = <&macaddr_art_0>;
		nvmem-cell-names = "mac-address";
		mac-address-increment = <1>;
		qca,no-eeprom;
		#gpio-cells = <2>;
		gpio-controller;
	};
};

&art {
	compatible = "nvmem-cells";
	#address-cells = <1>;
	#size-cells = <1>;

	macaddr_art_0: macaddr@0 {
		reg = <0x0 0x6>;
	};
};
