From b18f7a3c76cc764e58e9aabc3150a994e1d3f40b Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.com>
Date: Mon, 12 Jul 2021 15:15:44 +0100
Subject: [PATCH] ARM: dts: bcm2711: fold in the correct interrupt

The new vec node in bcm2711.dtsi should have the correct interrupt
number to start with, rather than include the bcm283x version and
patch it later.

Signed-off-by: Phil Elwell <phil@raspberrypi.com>
---
 arch/arm/boot/dts/bcm2711.dtsi | 6 +-----
 1 file changed, 1 insertion(+), 5 deletions(-)

--- a/arch/arm/boot/dts/bcm2711.dtsi
+++ b/arch/arm/boot/dts/bcm2711.dtsi
@@ -304,7 +304,7 @@
 			compatible = "brcm,bcm2711-vec";
 			reg = <0x7ec13000 0x1000>;
 			clocks = <&clocks BCM2835_CLOCK_VEC>;
-			interrupts = <2 27>;
+			interrupts = <GIC_SPI 123 IRQ_TYPE_LEVEL_HIGH>;
 			status = "disabled";
 		};
 
@@ -1106,7 +1106,3 @@
 &usb {
 	interrupts = <GIC_SPI 73 IRQ_TYPE_LEVEL_HIGH>;
 };
-
-&vec {
-	interrupts = <GIC_SPI 123 IRQ_TYPE_LEVEL_HIGH>;
-};
