// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "ar7100.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/mtd/partitions/uimage.h>

/ {
	aliases {
		led-boot = &led_power_orange;
		led-failsafe = &led_power_orange;
		led-running = &led_power_green;
		led-upgrade = &led_power_orange;
	};

	extosc: ref {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-output-names = "ref";
		clock-frequency = <40000000>;
	};

	reset-leds {
		compatible = "reset-leds";

		usb_led {
			label = "green:usb";
			resets = <&rst 12>;
			trigger-sources = <&usb_ohci_port>, <&usb_ehci_port>;
			linux,default-trigger = "usbport";
		};
	};

	leds {
		compatible = "gpio-leds";

		wps {
			label = "orange:wps";
			gpios = <&gpio 0 GPIO_ACTIVE_LOW>;
		};

		led_power_green: power_green {
			label = "green:power";
			gpios = <&gpio 2 GPIO_ACTIVE_LOW>;
		};

		led_power_orange: power_orange {
			label = "orange:power";
			gpios = <&gpio 1 GPIO_ACTIVE_LOW>;
			default-state = "on";
		};

		wps_green {
			label = "green:wps";
			gpios = <&gpio 4 GPIO_ACTIVE_LOW>;
		};

		wan_green {
			label = "green:wan";
			gpios = <&gpio 6 GPIO_ACTIVE_LOW>;
		};
	};

	ath9k-leds {
		compatible = "gpio-leds";

		wlan2g {
			label = "green:wlan2g";
			gpios = <&ath9k0 5 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};
		wlan5g {
			label = "blue:wlan5g";
			gpios = <&ath9k1 5 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1tpt";
		};
	};

	keys {
		compatible = "gpio-keys";

		wps {
			label = "wps";
			linux,code = <KEY_WPS_BUTTON>;
			gpios = <&gpio 3 GPIO_ACTIVE_LOW>;
		};

		reset {
			label = "reset";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 8 GPIO_ACTIVE_LOW>;
		};

		rfkill {
			label = "rfkill";
			linux,code = <KEY_RFKILL>;
			gpios = <&gpio 11 GPIO_ACTIVE_LOW>;
		};
	};

	rtl8366s {
		compatible = "realtek,rtl8366s";

		gpio-sda = <&gpio 5 GPIO_ACTIVE_HIGH>;
		gpio-sck = <&gpio 7 GPIO_ACTIVE_HIGH>;

		mdio-bus {
			#address-cells = <1>;
			#size-cells = <0>;
			status = "okay";

			phy-mask = <0x10>;

			phy4: ethernet-phy@4 {
				reg = <4>;
				phy-mode = "rgmii";
			};
		};
	};
};

&usb_phy {
	status = "okay";
};

&usb1 {
	#address-cells = <1>;
	#size-cells = <0>;
	status = "okay";

	usb_ohci_port: port@1 {
		reg = <1>;
		#trigger-source-cells = <0>;
	};
};

&usb2 {
	#address-cells = <1>;
	#size-cells = <0>;
	status = "okay";

	usb_ehci_port: port@1 {
		reg = <1>;
		#trigger-source-cells = <0>;
	};
};

&pcie0 {
	status = "okay";

	ath9k0: wifi@0,11 {
		compatible = "pci168c,0029";
		reg = <0x8800 0 0 0 0>;

		qca,no-eeprom;
		#gpio-cells = <2>;
		gpio-controller;

		/* all WNDR3700 variants have four antennae dedicated
		 * to the 2.4GHz radio. Two antennae are available for
		 * each chain. The following configuration is the
		 * default setting which taken from the vendor's wifi
		 * code for that radio.
		 *
		 * All possible options [GPIO6,GPIO7,GPIO8,GPIO9]:
		 *	[0,1,0,1], [0,1,1,0], [1,0,0,1], [1,0,1,0]
		 */
		antenna-demux {
			gpio-hog;
			line-name = "fixed antenna group 1";
			gpios = <6 GPIO_ACTIVE_LOW>,
				<7 GPIO_ACTIVE_HIGH>,
				<8 GPIO_ACTIVE_LOW>,
				<9 GPIO_ACTIVE_HIGH>;
			output-high;
		};
	};

	ath9k1: wifi@0,12 {
		compatible = "pci168c,0029";
		reg = <0x9000 0 0 0 0>;

		qca,no-eeprom;
		#gpio-cells = <2>;
		gpio-controller;
	};
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions: partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;
		};
	};
};

&eth0 {
	status = "okay";

	pll-data = <0x11110000 0x00001099 0x00991099>;

	fixed-link {
		speed = <1000>;
		full-duplex;
	};
};

&eth1 {
	status = "okay";

	pll-data = <0x11110000 0x00001099 0x00991099>;

	phy-handle = <&phy4>;
};
