From b74589474b5db6154cca49278df7fdccf92b6ab9 Mon Sep 17 00:00:00 2001
From: Dom Cobley <popcornmix@gmail.com>
Date: Mon, 11 Jan 2021 17:08:20 +0000
Subject: [PATCH] bcm2711: Remove old GIC interrupt

Now handled through aon_intr

Signed-off-by: Dom Cobley <popcornmix@gmail.com>
---
 arch/arm/boot/dts/bcm2711.dtsi | 2 --
 1 file changed, 2 deletions(-)

--- a/arch/arm/boot/dts/bcm2711.dtsi
+++ b/arch/arm/boot/dts/bcm2711.dtsi
@@ -353,7 +353,6 @@
 			ddc = <&ddc0>;
 			dmas = <&dma 10>;
 			dma-names = "audio-rx";
-			interrupts = <GIC_SPI 96 IRQ_TYPE_LEVEL_HIGH>;
 			status = "disabled";
 		};
 
@@ -401,7 +400,6 @@
 					  "wakeup", "hpd-connected", "hpd-removed";
 			dmas = <&dma 17>;
 			dma-names = "audio-rx";
-			interrupts = <GIC_SPI 96 IRQ_TYPE_LEVEL_HIGH>;
 			status = "disabled";
 		};
 
