From 787082ab9f7be4711e52f67c388535eda74a1269 Mon Sep 17 00:00:00 2001
From: Ilya Lipnitskiy <ilya.lipnitskiy@gmail.com>
Date: Thu, 22 Apr 2021 22:20:56 -0700
Subject: [PATCH] net: ethernet: mtk_eth_soc: fix build_skb cleanup

In case build_skb fails, call skb_free_frag on the correct pointer. Also
update the DMA structures with the new mapping before exiting, because
the mapping was successful

Suggested-by: Felix Fietkau <nbd@nbd.name>
Signed-off-by: Ilya Lipnitskiy <ilya.lipnitskiy@gmail.com>
Signed-off-by: David S. Miller <davem@davemloft.net>
---
 drivers/net/ethernet/mediatek/mtk_eth_soc.c | 5 +++--
 1 file changed, 3 insertions(+), 2 deletions(-)

--- a/drivers/net/ethernet/mediatek/mtk_eth_soc.c
+++ b/drivers/net/ethernet/mediatek/mtk_eth_soc.c
@@ -1325,9 +1325,9 @@ static int mtk_poll_rx(struct napi_struc
 		/* receive data */
 		skb = build_skb(data, ring->frag_size);
 		if (unlikely(!skb)) {
-			skb_free_frag(new_data);
+			skb_free_frag(data);
 			netdev->stats.rx_dropped++;
-			goto release_desc;
+			goto skip_rx;
 		}
 		skb_reserve(skb, NET_SKB_PAD + NET_IP_ALIGN);
 
@@ -1347,6 +1347,7 @@ static int mtk_poll_rx(struct napi_struc
 		skb_record_rx_queue(skb, 0);
 		napi_gro_receive(napi, skb);
 
+skip_rx:
 		ring->data[idx] = new_data;
 		rxd->rxd1 = (unsigned int)dma_addr;
 
