From 6731d2c9039fbe1ecf21915eab3acee0a999508a Mon Sep 17 00:00:00 2001
From: David Bauer <mail@david-bauer.net>
Date: Fri, 10 Jul 2020 21:38:20 +0200
Subject: [PATCH] rockchip: use system LED for OpenWrt

Use the SYS LED on the casing for showing system status.

This patch is kept separate from the NanoPi R2S support patch, as i plan
on submitting the device support upstream.

Signed-off-by: David Bauer <mail@david-bauer.net>
---
 arch/arm64/boot/dts/rockchip/rk3328-nanopi-r2s.dts | 9 ++++++++-
 1 file changed, 8 insertions(+), 1 deletion(-)

--- a/arch/arm64/boot/dts/rockchip/rk3328-nanopi-r2s.dts
+++ b/arch/arm64/boot/dts/rockchip/rk3328-nanopi-r2s.dts
@@ -13,6 +13,13 @@
 	model = "FriendlyElec NanoPi R2S";
 	compatible = "friendlyarm,nanopi-r2s", "rockchip,rk3328";
 
+	aliases {
+		led-boot = &sys_led;
+		led-failsafe = &sys_led;
+		led-running = &sys_led;
+		led-upgrade = &sys_led;
+	};
+
 	chosen {
 		stdout-path = "serial2:1500000n8";
 	};
