From 8ee4a5f4f40da60bb85e13d9dd218a3c9197e3e3 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Marek=20Beh=C3=BAn?= <kabel@kernel.org>
Date: Sun, 15 Nov 2020 14:59:22 +0100
Subject: ARM: dts: turris-omnia: update ethernet-phy node and handle name
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Use property name `phy-handle` instead of the deprecated `phy` to
connect eth2 to the PHY.
Rename the node from "phy@1" to "ethernet-phy@1", since "phy@1" is
incorrect according to device-tree bindings documentation.
Also remove the "ethernet-phy-id0141.0DD1" compatible string, it is not
needed. Kernel can read the PHY identifier itself.

Signed-off-by: Marek Behún <kabel@kernel.org>
Reviewed-by: Andrew Lunn <andrew@lunn.ch>
Cc: linux-arm-kernel@lists.infradead.org
Cc: Uwe Kleine-König <uwe@kleine-koenig.org>
Cc: Jason Cooper <jason@lakedaemon.net>
Cc: Gregory CLEMENT <gregory.clement@bootlin.com>
Cc: Andreas Färber <afaerber@suse.de>
Cc: Rob Herring <robh+dt@kernel.org>
Cc: devicetree@vger.kernel.org
Signed-off-by: Gregory CLEMENT <gregory.clement@bootlin.com>
---
 arch/arm/boot/dts/armada-385-turris-omnia.dts | 6 +++---
 1 file changed, 3 insertions(+), 3 deletions(-)

--- a/arch/arm/boot/dts/armada-385-turris-omnia.dts
+++ b/arch/arm/boot/dts/armada-385-turris-omnia.dts
@@ -156,7 +156,7 @@
 	 */
 	status = "okay";
 	phy-mode = "sgmii";
-	phy = <&phy1>;
+	phy-handle = <&phy1>;
 	phys = <&comphy5 2>;
 	sfp = <&sfp>;
 	buffer-manager = <&bm>;
@@ -387,9 +387,9 @@
 	pinctrl-0 = <&mdio_pins>;
 	status = "okay";
 
-	phy1: phy@1 {
+	phy1: ethernet-phy@1 {
 		status = "okay";
-		compatible = "ethernet-phy-id0141.0DD1", "ethernet-phy-ieee802.3-c22";
+		compatible = "ethernet-phy-ieee802.3-c22";
 		reg = <1>;
 		marvell,reg-init = <3 18 0 0x4985>;
 
