// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "mt7620a.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "iodata,wn-ac733gr3", "ralink,mt7620a-soc";
	model = "I-O DATA WN-AC733GR3";

	aliases {
		led-boot = &led_power;
		led-failsafe = &led_power;
		led-running = &led_power;
		led-upgrade = &led_power;
	};

	leds {
		compatible = "gpio-leds";

		led_power: power {
			label = "green:power";
			gpios = <&gpio0 7 GPIO_ACTIVE_LOW>;
			default-state = "on";
		};

		notification {
			label = "green:notification";
			gpios = <&gpio0 8 GPIO_ACTIVE_LOW>;
		};

		wlan2g {
			label = "green:wlan2g";
			gpios = <&gpio0 10 GPIO_ACTIVE_LOW>;
		};

		wlan5g {
			label = "green:wlan5g";
			gpios = <&gpio0 14 GPIO_ACTIVE_LOW>;
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			gpios = <&gpio0 1 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};

		wps {
			label = "wps";
			gpios = <&gpio0 2 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};

		router {
			label = "router";
			gpios = <&gpio0 12 GPIO_ACTIVE_LOW>;
			linux,code = <BTN_0>;
			linux,input-type = <EV_SW>;
		};

		auto {
			label = "auto";
			gpios = <&gpio0 13 GPIO_ACTIVE_LOW>;
			linux,code = <BTN_0>;
			linux,input-type = <EV_SW>;
		};
	};

	rtl8367rb {
		compatible = "realtek,rtl8367b";
		gpio-sda = <&gpio0 22 GPIO_ACTIVE_HIGH>;
		gpio-sck = <&gpio0 23 GPIO_ACTIVE_HIGH>;
		realtek,extif1 = <1 0 1 1 1 1 1 1 2>;
	};
};

&spi0 {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <10000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x0 0x30000>;
				read-only;
			};

			partition@30000 {
				label = "u-boot-env";
				reg = <0x30000 0x10000>;
				read-only;
			};

			factory: partition@40000 {
				label = "factory";
				reg = <0x40000 0x8000>;
				read-only;
			};

			iNIC_rf: partition@48000 {
				label = "iNIC_rf";
				reg = <0x48000 0x8000>;
				read-only;
			};

			partition@50000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x50000 0x6d4000>;
			};

			partition@724000 {
				label = "manufacture";
				reg = <0x724000 0x8c000>;
				read-only;
			};

			partition@7b0000 {
				label = "backup";
				reg = <0x7b0000 0x10000>;
				read-only;
			};

			partition@7c0000 {
				label = "storage";
				reg = <0x7c0000 0x40000>;
				read-only;
			};
		};
	};
};

&ethernet {
	pinctrl-names = "default";
	pinctrl-0 = <&rgmii1_pins>;

	nvmem-cells = <&macaddr_factory_4>;
	nvmem-cell-names = "mac-address";

	port@5 {
		status = "okay";
		mediatek,fixed-link = <1000 1 1 1>;
		phy-mode = "rgmii";
	};
};

&gpio0 {
	rtl8367rb_reset {
		gpio-hog;
		gpios = <0 GPIO_ACTIVE_HIGH>;
		output-high;
		line-name = "rtl8367rb-reset";
	};
};

&state_default {
	gpio {
		groups = "i2c", "uartf", "mdio";
		function = "gpio";
	};
};

&pcie {
	status = "okay";
};

&pcie0 {
	wifi@0,0 {
		compatible = "mediatek,mt76";
		reg = <0x0000 0 0 0 0>;
		mediatek,mtd-eeprom = <&iNIC_rf 0x0>;
		ieee80211-freq-limit = <5000000 6000000>;
	};
};

&wmac {
	ralink,mtd-eeprom = <&factory 0x0>;
};

&factory {
	compatible = "nvmem-cells";
	#address-cells = <1>;
	#size-cells = <1>;

	macaddr_factory_4: macaddr@4 {
		reg = <0x4 0x6>;
	};
};
