From e463f4a9d933d2d62a065bba356a9eb04a9f3ac0 Mon Sep 17 00:00:00 2001
From: Florin Chiculita <florinlaurentiu.chiculita@nxp.com>
Date: Tue, 11 Jun 2019 23:53:45 +0300
Subject: [PATCH] arm64: dts: lx2160a: update interrupt property for Aquantia
 phy

Update Aquantia AQR107 nodes interrupt property.

Signed-off-by: Florin Chiculita <florinlaurentiu.chiculita@nxp.com>
---
 arch/arm64/boot/dts/freescale/fsl-lx2160a-rdb.dts | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

--- a/arch/arm64/boot/dts/freescale/fsl-lx2160a-rdb.dts
+++ b/arch/arm64/boot/dts/freescale/fsl-lx2160a-rdb.dts
@@ -200,13 +200,13 @@
 	aquantia_phy1: ethernet-phy@4 {
 		/* AQR107 PHY - "compatible" property not strictly needed */
 		compatible = "ethernet-phy-ieee802.3-c45";
-		interrupts = <GIC_SPI 1 IRQ_TYPE_LEVEL_HIGH>;
+		interrupts = <GIC_SPI 2 IRQ_TYPE_LEVEL_HIGH>;
 		reg = <0x4>;
 	};
 	aquantia_phy2: ethernet-phy@5 {
 		/* AQR107 PHY - "compatible" property not strictly needed */
 		compatible = "ethernet-phy-ieee802.3-c45";
-		interrupts = <GIC_SPI 2 IRQ_TYPE_LEVEL_HIGH>;
+		interrupts = <GIC_SPI 3 IRQ_TYPE_LEVEL_HIGH>;
 		reg = <0x5>;
 	};
 };
