#include "rt3883.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "asus,rt-n56u", "ralink,rt3662-soc", "ralink,rt3883-soc";
	model = "Asus RT-N56U";

	aliases {
		led-boot = &led_power;
		led-failsafe = &led_power;
		led-running = &led_power;
		led-upgrade = &led_power;
	};

	flash@1c000000 {
		compatible = "cfi-flash";
		reg = <0x1c000000 0x800000>;
		bank-width = <2>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				reg = <0x0 0x0030000>;
				label = "u-boot";
				read-only;
			};

			partition@30000 {
				reg = <0x00030000 0x00010000>;
				label = "u-boot-env";
				read-only;
			};

			factory: partition@40000 {
				reg = <0x00040000 0x00010000>;
				label = "factory";
				read-only;
			};

			partition@50000 {
				compatible = "denx,uimage";
				reg = <0x00050000 0x007b0000>;
				label = "firmware";
			};
		};
	};

	rtl8367 {
		compatible = "realtek,rtl8367";
		gpio-sda = <&gpio0 1 GPIO_ACTIVE_HIGH>;
		gpio-sck = <&gpio0 2 GPIO_ACTIVE_HIGH>;
		realtek,extif1 = <1 0 1 1 1 1 1 1 2>;
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <100>;

		reset {
			label = "reset";
			gpios = <&gpio0 13 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};

		wps {
			label = "wps";
			gpios = <&gpio1 2 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_power: power {
			label = "blue:power";
			gpios = <&gpio0 0 GPIO_ACTIVE_LOW>;
		};

		lan {
			label = "blue:lan";
			gpios = <&gpio0 19 GPIO_ACTIVE_LOW>;
		};

		wan {
			label = "blue:wan";
			gpios = <&gpio1 3 GPIO_ACTIVE_LOW>;
		};

		usb {
			label = "blue:usb";
			gpios = <&gpio1 0 GPIO_ACTIVE_LOW>;
		};
	};
};

&gpio1 {
	status = "okay";
};

&state_default {
	gpio {
		groups = "spi", "i2c", "jtag", "uartf";
		function = "gpio";
	};
};

&ethernet {
	nvmem-cells = <&macaddr_factory_4>;
	nvmem-cell-names = "mac-address";

	port@0 {
		mediatek,fixed-link = <1000 1 1 1>;
	};
};

&pci {
	status = "okay";
};

&pci1 {
	status = "okay";

	wifi@0,0 {
		compatible = "pci1814,3091";
		reg = <0x10000 0 0 0 0>;
		ralink,mtd-eeprom = <&factory 0x8000>;
	};
};

&wmac {
	status = "okay";
	ralink,2ghz = <0>;
	ralink,mtd-eeprom = <&factory 0x0>;
};

&ehci {
	status = "okay";
};

&ohci {
	status = "okay";
};

&factory {
	compatible = "nvmem-cells";
	#address-cells = <1>;
	#size-cells = <1>;

	macaddr_factory_4: macaddr@4 {
		reg = <0x4 0x6>;
	};
};
