// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "qca956x.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	model = "Xiaomi AIoT AC2350";
	compatible = "xiaomi,aiot-ac2350", "qca,qca9563";

	aliases {
		label-mac-device = &eth0;

		led-boot = &led_system_orange;
		led-failsafe = &led_system_orange;
		led-running = &led_system_blue;
		led-upgrade = &led_system_orange;
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 2 GPIO_ACTIVE_HIGH>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_system_blue: system_blue {
			label = "blue:system";
			gpios = <&gpio 5 GPIO_ACTIVE_LOW>;
		};

		led_system_orange: system_orange {
			label = "orange:system";
			gpios = <&gpio 7 GPIO_ACTIVE_LOW>;
		};

		wan_blue {
			label = "blue:wan";
			gpios = <&gpio 8 GPIO_ACTIVE_LOW>;
		};

		wan_orange {
			label = "orange:wan";
			gpios = <&gpio 15 GPIO_ACTIVE_LOW>;
		};
	};

	gpio-export {
		compatible = "gpio-export";

		wps {
			gpio-export,name = "wps";
			gpio-export,output = <0>;
			gpios = <&gpio 1 GPIO_ACTIVE_HIGH>;
		};

		usb-reset {
			gpio-export,name = "usb-reset";
			gpio-export,output = <0>;
			gpios = <&gpio 19 GPIO_ACTIVE_HIGH>;
		};
	};
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <50000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "Bootloader";
				reg = <0x0 0x30000>;
				read-only;
			};

			partition@30000 {
				label = "Nvram";
				reg = <0x30000 0x10000>;
			};

			partition@40000 {
				label = "Bdata";
				reg = <0x40000 0x10000>;
				read-only;
			};

			partition@50000 {
				label = "crash";
				reg = <0x50000 0x10000>;
				read-only;
			};

			art: partition@60000 {
				label = "art";
				reg = <0x60000 0x10000>;
				read-only;
			};

			partition@70000 {
				label = "cfg_bak";
				reg = <0x70000 0x20000>;
				read-only;
			};

			partition@90000 {
				label = "overlay";
				reg = <0x90000 0x170000>;
				read-only;
			};

			partition@200000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x200000 0xe00000>;
			};
		};
	};
};

&mdio0 {
	status = "okay";

	phy-mask = <0x1>;

	phy0: ethernet-phy@0 {
		reg = <0>;
		phy-mode = "sgmii";

		qca,ar8327-initvals = <
			0x04 0x00000080 /* PORT0 PAD MODE CTRL */
			0x08 0x01000000 /* PORT5 PAD MODE CTRL */
			0x0c 0x00000000 /* PORT6 PAD MODE CTRL */
			0x10 0x602613a0 /* POWER_ON_STRAP */
			0x50 0xcf35cf35 /* LED_CTRL0 */
			0x54 0xca35ca35 /* LED_CTRL1 */
			0x58 0xc935c935 /* LED_CTRL2 */
			0x5c 0x03ffff00 /* LED_CTRL3 */
			0x7c 0x000000fe /* PORT0_STATUS */
			0x94 0x000010c2 /* PORT6_STATUS */
			0xe0 0xc74164de /* SGMII_CTRL */
		>;
	};
};

&eth0 {
	status = "okay";

	phy-mode = "sgmii";
	phy-handle = <&phy0>;

	nvmem-cells = <&macaddr_art_0>;
	nvmem-cell-names = "mac-address";
};

&wmac {
	status = "okay";

	mtd-cal-data = <&art 0x1000>;
};

&pcie {
	status = "okay";
};

&art {
	compatible = "nvmem-cells";
	#address-cells = <1>;
	#size-cells = <1>;

	macaddr_art_0: macaddr@0 {
		reg = <0x0 0x6>;
	};
};
