// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "qca955x.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	chosen {
		/delete-property/ bootargs;
	};

	aliases {
		serial0 = &uart;
		led-boot = &led_status_green;
		led-failsafe = &led_status_green;
		led-running = &led_status_green;
		led-upgrade = &led_status_green;
		label-mac-device = &eth0;
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 17 GPIO_ACTIVE_LOW>;
		};
	};

	leds {
		compatible = "gpio-leds";

		status_blue {
			label = "blue:status";
			gpios = <&gpio 13 GPIO_ACTIVE_HIGH>;
		};

		status_red {
			label = "red:status";
			gpios = <&gpio 22 GPIO_ACTIVE_HIGH>;
		};

		led_status_green: status_green {
			label = "green:status";
			gpios = <&gpio 23 GPIO_ACTIVE_HIGH>;
		};
	};

	watchdog {
		compatible = "linux,wdt-gpio";
		gpios = <&gpio 16 GPIO_ACTIVE_LOW>;
		hw_algo = "toggle";
		/* hw_margin_ms is actually 300s but driver limits it to 60s */
		hw_margin_ms = <60000>;
		always-running;
	};
};

&usb_phy1 {
	status = "okay";
};

&usb1 {
	status = "okay";
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <40000000>;

		/* partitions are passed via bootloader */
		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x000000 0x040000>;
				read-only;
			};

			partition@40000 {
				label = "u-boot-env";
				reg = <0x040000 0x010000>;
			};

			partition@50000 {
				label = "custom";
				reg = <0x050000 0x060000>;
				read-only;
			};

			partition@b0000 {
				label = "inactive";
				reg = <0x0b0000 0x7a0000>;
			};

			partition@850000 {
				label = "inactive2";
				reg = <0x850000 0x7a0000>;
			};

			art: partition@ff0000 {
				label = "ART";
				reg = <0xff0000 0x010000>;
				read-only;
			};
		};
	};
};

&mdio0 {
	status = "okay";

	phy-mask = <0x6>;

	phy1: ethernet-phy@1 {
		reg = <1>;
		eee-broken-100tx;
		eee-broken-1000t;
	};

	phy2: ethernet-phy@2 {
		reg = <2>;
		eee-broken-100tx;
		eee-broken-1000t;
		at803x-override-sgmii-link-check;
	};
};

&eth0 {
	status = "okay";

	pll-data = <0x82000101 0x80000101 0x80001313>;

	nvmem-cells = <&macaddr_art_0>;
	nvmem-cell-names = "mac-address";

	phy-mode = "rgmii-id";
	phy-handle = <&phy1>;

	gmac-config {
		device = <&gmac>;
		rgmii-enabled = <1>;
		rxd-delay = <3>;
		rxdv-delay = <3>;
		txd-delay = <0>;
		txen-delay = <0>;
	};
};

&eth1 {
	status = "okay";

	pll-data = <0x03000101 0x80000101 0x80001313>;

	nvmem-cells = <&macaddr_art_6>;
	nvmem-cell-names = "mac-address";

	qca955x-sgmii-fixup;

	phy-handle = <&phy2>;
};

&wmac {
	status = "okay";

	mtd-cal-data = <&art 0x1000>;
	nvmem-cells = <&macaddr_art_0>;
	nvmem-cell-names = "mac-address";
	mac-address-increment = <2>;
};

&pcie0 {
	status = "okay";
};

&art {
	compatible = "nvmem-cells";
	#address-cells = <1>;
	#size-cells = <1>;

	macaddr_art_0: macaddr@0 {
		reg = <0x0 0x6>;
	};

	macaddr_art_6: macaddr@6 {
		reg = <0x6 0x6>;
	};
};
