From 10c1e714a68b45b124157aa02d80abe244a2a61a Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?=C3=81lvaro=20Fern=C3=A1ndez=20Rojas?= <noltari@gmail.com>
Date: Wed, 17 Jun 2020 12:50:34 +0200
Subject: [PATCH 2/9] dt-bindings: reset: add BCM6345 reset controller bindings
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Add device tree binding documentation for BCM6345 reset controller.

Signed-off-by: Álvaro Fernández Rojas <noltari@gmail.com>
Reviewed-by: Florian Fainelli <f.fainelli@gmail.com>
Reviewed-by: Rob Herring <robh@kernel.org>
Signed-off-by: Thomas Bogendoerfer <tsbogend@alpha.franken.de>
---
 .../bindings/reset/brcm,bcm6345-reset.yaml    | 37 +++++++++++++++++++
 1 file changed, 37 insertions(+)
 create mode 100644 Documentation/devicetree/bindings/reset/brcm,bcm6345-reset.yaml

--- /dev/null
+++ b/Documentation/devicetree/bindings/reset/brcm,bcm6345-reset.yaml
@@ -0,0 +1,37 @@
+# SPDX-License-Identifier: (GPL-2.0-only OR BSD-2-Clause)
+%YAML 1.2
+---
+$id: "http://devicetree.org/schemas/reset/brcm,bcm6345-reset.yaml#"
+$schema: "http://devicetree.org/meta-schemas/core.yaml#"
+
+title: BCM6345 reset controller
+
+description: This document describes the BCM6345 reset controller.
+
+maintainers:
+  - Álvaro Fernández Rojas <noltari@gmail.com>
+
+properties:
+  compatible:
+    const: brcm,bcm6345-reset
+
+  reg:
+    maxItems: 1
+
+  "#reset-cells":
+    const: 1
+
+required:
+  - compatible
+  - reg
+  - "#reset-cells"
+
+additionalProperties: false
+
+examples:
+  - |
+    reset-controller@10000010 {
+      compatible = "brcm,bcm6345-reset";
+      reg = <0x10000010 0x4>;
+      #reset-cells = <1>;
+    };
