From f290455548d9e9ea5f03464d229d08a854a9fb37 Mon Sep 17 00:00:00 2001
From: popcornmix <popcornmix@gmail.com>
Date: Wed, 1 Apr 2020 11:22:44 +0100
Subject: [PATCH] bcmgenet: Disable skip_umac_reset by default

Possible fixed upstream by 'net: bcmgenet: keep MAC in reset until PHY is up'

Signed-off-by: popcornmix <popcornmix@gmail.com>
---
 drivers/net/ethernet/broadcom/genet/bcmgenet.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/net/ethernet/broadcom/genet/bcmgenet.c
+++ b/drivers/net/ethernet/broadcom/genet/bcmgenet.c
@@ -67,7 +67,7 @@
 
 /* Forward declarations */
 static void bcmgenet_set_rx_mode(struct net_device *dev);
-static bool skip_umac_reset = true;
+static bool skip_umac_reset = false;
 module_param(skip_umac_reset, bool, 0444);
 MODULE_PARM_DESC(skip_umac_reset, "Skip UMAC reset step");
 
