#include "ar9.dtsi"

#include <dt-bindings/input/input.h>

/ {
	compatible = "avm,fritz7320", "lantiq,xway", "lantiq,ar9";
	model = "AVM FRITZ!Box 7320";

	chosen {
		bootargs = "console=ttyLTQ0,115200";
	};

	aliases {
		led-boot = &power;
		led-failsafe = &power;
		led-running = &power;
		led-upgrade = &power;

		led-dsl = &info_green;
		led-wifi = &wlan;
	};

	memory@0 {
		device_type = "memory";
		reg = <0x0 0x4000000>;
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <100>;

		rfkill {
			label = "rfkill";
			gpios = <&gpio 1 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RFKILL>;
		};
		dect {
			label = "dect";
			gpios = <&gpio 2 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_PHONE>;
		};
	};

	leds {
		compatible = "gpio-leds";
		power: power {
			label = "green:power";
			gpios = <&gpio 44 GPIO_ACTIVE_LOW>;
			default-state = "keep";
		};
		voice {
			label = "green:fon";
			gpios = <&gpio 47 GPIO_ACTIVE_LOW>;
		};
		dect {
			label = "green:dect";
			gpios = <&gpio 38 GPIO_ACTIVE_LOW>;
		};
		wlan: wlan {
			label = "green:wlan";
			gpios = <&gpio 37 GPIO_ACTIVE_LOW>;
		};
		info_green: info_green {
			label = "green:info";
			gpios = <&gpio 35 GPIO_ACTIVE_LOW>;
		};
		info_red {
			label = "red:info";
			gpios = <&gpio 45 GPIO_ACTIVE_LOW>;
		};
	};

	usb0_vbus: regulator-usb0-vbus {
		compatible = "regulator-fixed";

		regulator-name = "USB0_VBUS";

		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;

		gpio = <&gpio 50 GPIO_ACTIVE_HIGH>;
		enable-active-high;
	};

	usb1_vbus: regulator-usb1-vbus {
		compatible = "regulator-fixed";

		regulator-name = "USB1_VBUS";

		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;

		gpio = <&gpio 51 GPIO_ACTIVE_HIGH>;
		enable-active-high;
	};
};

&gsw {
	phy-mode = "mii";
	nvmem-cells = <&macaddr_ath9k_cal_a91>;
	nvmem-cell-names = "mac-address";
	mac-address-increment = <(-2)>;
};

&gpio {
	pinctrl-names = "default";
	pinctrl-0 = <&state_default>;

	state_default: pinmux {
		usb0_vbus {
			lantiq,pins = "io50";
			lantiq,pull = <0>;
			lantiq,open-drain = <0>;
			lantiq,output = <1>;
		};
		usb1_vbus {
			lantiq,pins = "io51";
			lantiq,pull = <0>;
			lantiq,open-drain = <0>;
			lantiq,output = <1>;
		};
	};
};

&localbus {
	flash@0 {
		compatible = "lantiq,nor";
		bank-width = <2>;
		reg = <0 0x0 0x1000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			ath9k_cal: partition@0 {
				label = "urlader";
				reg = <0x00000 0x20000>;
				read-only;
			};

			partition@20000 {
				label = "firmware";
				reg = <0x20000 0xf60000>;
			};

			partition@f80000 {
				label = "tffs (1)";
				reg = <0xf80000 0x40000>;
				read-only;
			};

			partition@fc0000 {
				label = "tffs (2)";
				reg = <0xfc0000 0x40000>;
				read-only;
			};
		};
	};
};

&pci0 {
	status = "okay";

	pinctrl-0 = <&pci_gnt1_pins>, <&pci_gnt2_pins>,
		    <&pci_gnt3_pins>, <&pci_gnt4_pins>,
		    <&pci_req1_pins>, <&pci_req2_pins>,
		    <&pci_req3_pins>, <&pci_req4_pins>;

	req-mask = <0xf>;
	gpio-reset = <&gpio 21 GPIO_ACTIVE_HIGH>;

	wifi@0,0 {
		compatible = "pci0,0";
		reg = <0x7000 0 0 0 0>;
		qca,no-eeprom; /* load from ath9k-eeprom-pci-0000:00:0e.0.bin */
	};
};

&usb_phy0 {
	status = "okay";
};

&usb_phy1 {
	status = "okay";
};

&usb0 {
	status = "okay";
	vbus-supply = <&usb0_vbus>;
};

&usb1 {
	status = "okay";
	vbus-supply = <&usb1_vbus>;
};

&ath9k_cal {
	compatible = "nvmem-cells";
	#address-cells = <1>;
	#size-cells = <1>;

	macaddr_ath9k_cal_a91: macaddr@a91 {
		reg = <0xa91 0x6>;
	};
};
