// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "qca956x.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	aliases {
		led-boot = &led_power_amber;
		led-failsafe = &led_power_amber;
		led-running = &led_power_green;
		led-upgrade = &led_power_amber;
		label-mac-device = &eth0;
	};

	keys {
		compatible = "gpio-keys";

		wps {
			label = "wps";
			linux,code = <KEY_WPS_BUTTON>;
			gpios = <&gpio 1 GPIO_ACTIVE_LOW>;
		};

		reset {
			label = "reset";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 2 GPIO_ACTIVE_LOW>;
		};
	};

	ath9k-keys {
		compatible = "gpio-keys-polled";
		poll-interval = <20>;

		rfkill {
			label = "rfkill";
			linux,code = <KEY_RFKILL>;
			gpios = <&ath9k 9 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};
	};

	leds: leds {
		compatible = "gpio-leds";

		pinctrl-names = "default";
		pinctrl-0 = <&jtag_disable_pins>;

		led_power_green: power_green {
			label = "green:power";
			gpios = <&gpio 5 GPIO_ACTIVE_LOW>;
		};

		led_power_amber: power_amber {
			label = "amber:power";
			gpios = <&gpio 6 GPIO_ACTIVE_LOW>;
			default-state = "keep";
		};

		wan_green {
			label = "green:wan";
			gpios = <&gpio 17 GPIO_ACTIVE_LOW>;
		};

		wan_amber {
			label = "amber:wan";
			gpios = <&gpio 16 GPIO_ACTIVE_LOW>;
		};

		wlan2g_green {
			label = "green:wlan2g";
			gpios = <&gpio 19 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};

		wps_green {
			label = "green:wps";
			gpios = <&gpio 15 GPIO_ACTIVE_LOW>;
		};
	};

	ath9k-leds {
		compatible = "gpio-leds";

		wlan5g_blue {
			label = "blue:wlan5g";
			gpios = <&ath9k 7 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1tpt";
		};
	};
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x0 0x40000>;
				read-only;
			};

			partition@40000 {
				label = "u-boot-env";
				reg = <0x40000 0x10000>;
			};

			partition@50000 {
				label = "caldata_backup";
				reg = <0x50000 0x10000>;
				read-only;
			};

			partition@60000 {
				label = "config";
				reg = <0x60000 0x10000>;
			};

			partition@70000 {
				label = "traffic_meter";
				reg = <0x70000 0x10000>;
			};

			partition@80000 {
				label = "pot";
				reg = <0x80000 0x10000>;
			};

			partition@90000 {
				label = "reserved";
				reg = <0x90000 0x160000>;
			};

			caldata: partition@1f0000 {
				label = "caldata";
				reg = <0x1f0000 0x10000>;
				read-only;
			};
		};
	};

	flash@1 {
		compatible = "spi-nand";
		reg = <1>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "kernel";
				reg = <0x0 0x400000>;
			};

			partition@400000 {
				label = "ubi";
				reg = <0x400000 0x7c00000>;
			};
		};
	};
};

&mdio0 {
	status = "okay";

	phy-mask = <0>;

	phy0: ethernet-phy@0 {
		reg = <0>;
		phy-mode = "sgmii";
		qca,mib-poll-interval = <500>;

		qca,ar8327-initvals = <
			0x04 0x00000080	/* PORT0 PAD MODE CTRL */
			0x10 0x81000080	/* POWER_ON_STRAP */
			0x50 0xcc35cc35	/* LED_CTRL0 */
			0x54 0xcb37cb37	/* LED_CTRL1 */
			0x58 0x00000000	/* LED_CTRL2 */
			0x5c 0x00f3cf00	/* LED_CTRL3 */
			0x7c 0x0000007e	/* PORT0_STATUS */
			0x94 0x00000200 /* PORT6_STATUS */
			>;
	};
};

&eth0 {
	status = "okay";

	pll-data = <0x03000101 0x00000101 0x00001919>;

	nvmem-cells = <&macaddr_caldata_0>;
	nvmem-cell-names = "mac-address";

	phy-mode = "sgmii";
	phy-handle = <&phy0>;
};

&wmac {
	status = "okay";

	nvmem-cells = <&macaddr_caldata_0>;
	nvmem-cell-names = "mac-address";
	qca,no-eeprom;
};

&pcie {
	status = "okay";

	ath9k: wifi@0,0 {
		/* chip is AR9580, override bogus PCI ID 168c:abcd */
		compatible = "pci168c,0033";
		reg = <0x0000 0 0 0 0>;
		nvmem-cells = <&macaddr_caldata_c>;
		nvmem-cell-names = "mac-address";
		qca,no-eeprom;
		qca,gpio-mask=<0xf6ff>;	/* unmask pin 9 for RFKILL button */
		#gpio-cells = <2>;
		gpio-controller;
	};
};

&usb_phy0 {
	status = "okay";
};

&usb0 {
	#address-cells = <1>;
	#size-cells = <0>;
	status = "okay";

	hub_port0: port@1 {
		reg = <1>;
		#trigger-source-cells = <0>;
	};
};

&caldata {
	compatible = "nvmem-cells";
	#address-cells = <1>;
	#size-cells = <1>;

	macaddr_caldata_0: macaddr@0 {
		reg = <0x0 0x6>;
	};

	macaddr_caldata_c: macaddr@c {
		reg = <0xc 0x6>;
	};
};
