From 9ec25ef84832209a8326f9a71fe3ba14f4bcf301 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Marek=20Beh=C3=BAn?= <kabel@kernel.org>
Date: Sun, 15 Nov 2020 14:59:18 +0100
Subject: ARM: dts: turris-omnia: add comphy handle to eth2
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

The eth2 controller on Turris Omnia is connected to SerDes. For SFP to
be able to switch between 1G and 2.5G modes the comphy link has to be
defined.

Signed-off-by: Marek Behún <kabel@kernel.org>
Fixes: f3a6a9f3704a ("ARM: dts: add description for Armada 38x ...")
Reviewed-by: Andrew Lunn <andrew@lunn.ch>
Reviewed-by: Andreas Färber <afaerber@suse.de>
Cc: linux-arm-kernel@lists.infradead.org
Cc: Uwe Kleine-König <uwe@kleine-koenig.org>
Cc: Jason Cooper <jason@lakedaemon.net>
Cc: Gregory CLEMENT <gregory.clement@bootlin.com>
Cc: Rob Herring <robh+dt@kernel.org>
Cc: devicetree@vger.kernel.org
Signed-off-by: Gregory CLEMENT <gregory.clement@bootlin.com>
---
 arch/arm/boot/dts/armada-385-turris-omnia.dts | 1 +
 1 file changed, 1 insertion(+)

--- a/arch/arm/boot/dts/armada-385-turris-omnia.dts
+++ b/arch/arm/boot/dts/armada-385-turris-omnia.dts
@@ -129,6 +129,7 @@
 	status = "okay";
 	phy-mode = "sgmii";
 	phy = <&phy1>;
+	phys = <&comphy5 2>;
 	buffer-manager = <&bm>;
 	bm,pool-long = <2>;
 	bm,pool-short = <3>;
