From d0df79e13ab947367b86d7861e34f85aa6aad020 Mon Sep 17 00:00:00 2001
From: Dom Cobley <popcornmix@gmail.com>
Date: Sun, 24 Jan 2021 15:44:10 +0000
Subject: [PATCH] vc4/drm: Avoid full hdmi audio fifo writes

We are getting occasional VC4_HD_MAI_CTL_ERRORF in
HDMI_MAI_CTL which seem to correspond with audio dropouts.

Reduce the threshold where we deassert DREQ to avoid the fifo overfilling

Signed-off-by: Dom Cobley <popcornmix@gmail.com>
---
 drivers/gpu/drm/vc4/vc4_hdmi.c | 8 ++++----
 1 file changed, 4 insertions(+), 4 deletions(-)

--- a/drivers/gpu/drm/vc4/vc4_hdmi.c
+++ b/drivers/gpu/drm/vc4/vc4_hdmi.c
@@ -1294,10 +1294,10 @@ static int vc4_hdmi_audio_prepare(struct
 
 	/* Set the MAI threshold */
 	HDMI_WRITE(HDMI_MAI_THR,
-		   VC4_SET_FIELD(0x10, VC4_HD_MAI_THR_PANICHIGH) |
-		   VC4_SET_FIELD(0x10, VC4_HD_MAI_THR_PANICLOW) |
-		   VC4_SET_FIELD(0x10, VC4_HD_MAI_THR_DREQHIGH) |
-		   VC4_SET_FIELD(0x10, VC4_HD_MAI_THR_DREQLOW));
+		   VC4_SET_FIELD(0x08, VC4_HD_MAI_THR_PANICHIGH) |
+		   VC4_SET_FIELD(0x08, VC4_HD_MAI_THR_PANICLOW) |
+		   VC4_SET_FIELD(0x06, VC4_HD_MAI_THR_DREQHIGH) |
+		   VC4_SET_FIELD(0x08, VC4_HD_MAI_THR_DREQLOW));
 
 	HDMI_WRITE(HDMI_MAI_CONFIG,
 		   VC4_HDMI_MAI_CONFIG_BIT_REVERSE |
