--- a/arch/mips/include/asm/mach-bcm63xx/bcm63xx_dev_enet.h
+++ b/arch/mips/include/asm/mach-bcm63xx/bcm63xx_dev_enet.h
@@ -79,6 +79,9 @@ struct bcm63xx_enetsw_port {
 	int		force_speed;
 	int		force_duplex_full;
 
+	int		mii_override;
+	int		timing_sel;
+
 	const char	*name;
 };
 
--- a/drivers/net/ethernet/broadcom/bcm63xx_enet.c
+++ b/drivers/net/ethernet/broadcom/bcm63xx_enet.c
@@ -2232,6 +2232,10 @@ static int bcm_enetsw_open(struct net_de
 
 		rgmii_ctrl = enetsw_readb(priv, ENETSW_RGMII_CTRL_REG(i));
 		rgmii_ctrl |= ENETSW_RGMII_CTRL_GMII_CLK_EN;
+		if (priv->used_ports[i].mii_override)
+			rgmii_ctrl |= ENETSW_RGMII_CTRL_MII_OVERRIDE_EN;
+		if (priv->used_ports[i].timing_sel)
+			rgmii_ctrl |= ENETSW_RGMII_CTRL_TIMING_SEL_EN;
 		enetsw_writeb(priv, rgmii_ctrl, ENETSW_RGMII_CTRL_REG(i));
 	}
 
