// SPDX-License-Identifier: BSD-3-Clause
/*
 *  Copyright(c) 2017 Kristian Evensen <kristian.evensen@gmail.com>.
 *  Copyright(c) 2017 Piotr Dymacz <pepe2k@gmail.com>.
 *  All rights reserved.
 */

#include "mt7628an.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "unielec,u7628-01", "mediatek,mt7628an-soc";

	aliases {
		led-boot = &led_power;
		led-failsafe = &led_power;
		led-running = &led_power;
		led-upgrade = &led_power;
	};

	chosen {
		bootargs = "console=ttyS0,115200";
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			gpios = <&gpio 38 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_power: power {
			label = "green:power";
			gpios = <&gpio 44 GPIO_ACTIVE_LOW>;
		};

		wlan {
			label = "green:wlan";
			gpios = <&gpio 11 GPIO_ACTIVE_LOW>;
		};

		wan {
			label = "green:wan";
			gpios = <&gpio 43 GPIO_ACTIVE_LOW>;
		};

		lan1 {
			label = "green:lan1";
			gpios = <&gpio 42 GPIO_ACTIVE_LOW>;
		};

		lan2 {
			label = "green:lan2";
			gpios = <&gpio 41 GPIO_ACTIVE_LOW>;
		};

		lan3 {
			label = "green:lan3";
			gpios = <&gpio 40 GPIO_ACTIVE_LOW>;
		};

		lan4 {
			label = "green:lan4";
			gpios = <&gpio 39 GPIO_ACTIVE_LOW>;
		};

		usb {
			label = "green:usb";
			gpios = <&gpio 37 GPIO_ACTIVE_LOW>;
			trigger-sources = <&ohci_port1>, <&ehci_port1>;
			linux,default-trigger = "usbport";
		};
	};
};

&pcie {
	status = "okay";
};

&wmac {
	status = "okay";

	mediatek,mtd-eeprom = <&factory 0x0>;
};

&state_default {
	gpio {
		groups = "gpio", "p0led_an", "p1led_an", "p2led_an", "p3led_an", "p4led_an", "refclk", "wdt", "wled_an";
		function = "gpio";
	};
};
