From 4bdd40849632608d5cb7d3a64380cd76e7eea07b Mon Sep 17 00:00:00 2001
From: Jonas Gorski <jonas.gorski@gmail.com>
Date: Wed, 27 Jul 2016 11:33:56 +0200
Subject: [PATCH 02/16] Documentation: add BCM6328 pincontroller binding
 documentation

Add binding documentation for the pincontrol core found in BCM6328 SoCs.

Signed-off-by: Jonas Gorski <jonas.gorski@gmail.com>
---
 .../bindings/pinctrl/brcm,bcm6328-pinctrl.txt      | 61 ++++++++++++++++++++++
 1 file changed, 61 insertions(+)
 create mode 100644 Documentation/devicetree/bindings/pinctrl/brcm,bcm6328-pinctrl.txt

--- /dev/null
+++ b/Documentation/devicetree/bindings/pinctrl/brcm,bcm6328-pinctrl.txt
@@ -0,0 +1,61 @@
+* Broadcom BCM6328 pin controller
+
+Required properties:
+- compatible: Must be "brcm,bcm6328-pinctrl".
+- reg: Register specifies of dirout, dat, mode, mux registers.
+- reg-names: Must be "dirout", "dat", "mode", "mux".
+- gpio-controller: Identifies this node as a GPIO controller.
+- #gpio-cells: Must be <2>
+
+Example:
+
+pinctrl: pin-controller@10000080 {
+	compatible = "brcm,bcm6328-pinctrl";
+	reg = <0x10000080 0x8>,
+	      <0x10000088 0x8>,
+	      <0x10000098 0x4>,
+	      <0x1000009c 0xc>;
+	reg-names = "dirout", "dat", "mode", "mux";
+
+	gpio-controller;
+	#gpio-cells = <2>;
+};
+
+Available pins/groups and functions:
+
+name		pins	functions
+-----------------------------------------------------------
+gpio0		0	led
+gpio1		1	led
+gpio2		2	led
+gpio3		3	led
+gpio4		4	led
+gpio5		5	led
+gpio6		6	led, serial_led_data
+gpio7		7	led, serial_led_clk
+gpio8		8	led
+gpio9		9	led
+gpio10		10	led
+gpio11		11	led
+gpio12		12	led
+gpio13		13	led
+gpio14		14	led
+gpio15		15	led
+gpio16		16	led, pcie_clkreq
+gpio17		17	led
+gpio18		18	led
+gpio19		19	led
+gpio20		20	led
+gpio21		21	led
+gpio22		22	led
+gpio23		23	led
+gpio24		24	-
+gpio25		25	ephy0_act_led
+gpio26		26	ephy1_act_led
+gpio27		27	ephy2_act_led
+gpio28		28	ephy3_act_led
+gpio29		29	-
+gpio30		30	-
+gpio31		31	-
+hsspi_cs1	-	hsspi_cs1
+usb_port1	-	usb_host_port, usb_device_port
