From 1e6a19ca5f275155a4dd1961d351306b589b11a0 Mon Sep 17 00:00:00 2001
From: Maxime Ripard <maxime@cerno.tech>
Date: Mon, 26 Apr 2021 14:42:26 +0200
Subject: [PATCH] drm/vc4: Register HDMI codec

The hdmi-codec brings a lot of advanced features, including the HDMI
channel mapping. Let's use it in our driver instead of our own codec.

Signed-off-by: Maxime Ripard <maxime@cerno.tech>
---
 drivers/gpu/drm/vc4/Kconfig    |   1 +
 drivers/gpu/drm/vc4/vc4_hdmi.c | 311 +++++++++------------------------
 drivers/gpu/drm/vc4/vc4_hdmi.h |   3 +-
 3 files changed, 84 insertions(+), 231 deletions(-)

--- a/drivers/gpu/drm/vc4/Kconfig
+++ b/drivers/gpu/drm/vc4/Kconfig
@@ -12,6 +12,7 @@ config DRM_VC4
 	select SND_PCM
 	select SND_PCM_ELD
 	select SND_SOC_GENERIC_DMAENGINE_PCM
+	select SND_SOC_HDMI_CODEC
 	select DRM_MIPI_DSI
 	help
 	  Choose this option if you have a system that has a Broadcom
--- a/drivers/gpu/drm/vc4/vc4_hdmi.c
+++ b/drivers/gpu/drm/vc4/vc4_hdmi.c
@@ -47,6 +47,7 @@
 #include <linux/reset.h>
 #include <sound/asoundef.h>
 #include <sound/dmaengine_pcm.h>
+#include <sound/hdmi-codec.h>
 #include <sound/pcm_drm_eld.h>
 #include <sound/pcm_params.h>
 #include <sound/soc.h>
@@ -95,6 +96,12 @@
 # define VC4_HD_M_ENABLE			BIT(0)
 
 #define CEC_CLOCK_FREQ 40000
+#define HDMI_14_MAX_TMDS_CLK   (340 * 1000 * 1000)
+
+static bool vc4_hdmi_mode_needs_scrambling(const struct drm_display_mode *mode)
+{
+	return (mode->clock * 1000) > HDMI_14_MAX_TMDS_CLK;
+}
 
 static int vc4_hdmi_debugfs_regs(struct seq_file *m, void *unused)
 {
@@ -472,16 +479,10 @@ static void vc4_hdmi_set_spd_infoframe(s
 static void vc4_hdmi_set_audio_infoframe(struct drm_encoder *encoder)
 {
 	struct vc4_hdmi *vc4_hdmi = encoder_to_vc4_hdmi(encoder);
+	struct hdmi_audio_infoframe *audio = &vc4_hdmi->audio.infoframe;
 	union hdmi_infoframe frame;
-	int ret;
-
-	ret = hdmi_audio_infoframe_init(&frame.audio);
-
-	frame.audio.coding_type = HDMI_AUDIO_CODING_TYPE_STREAM;
-	frame.audio.sample_frequency = HDMI_AUDIO_SAMPLE_FREQUENCY_STREAM;
-	frame.audio.sample_size = HDMI_AUDIO_SAMPLE_SIZE_STREAM;
-	frame.audio.channels = vc4_hdmi->audio.channels;
 
+	memcpy(&frame.audio, audio, sizeof(*audio));
 	vc4_hdmi_write_infoframe(encoder, &frame);
 }
 
@@ -1214,18 +1215,10 @@ static inline struct vc4_hdmi *dai_to_hd
 	return snd_soc_card_get_drvdata(card);
 }
 
-static int vc4_hdmi_audio_startup(struct snd_pcm_substream *substream,
-				  struct snd_soc_dai *dai)
+static int vc4_hdmi_audio_startup(struct device *dev, void *data)
 {
-	struct vc4_hdmi *vc4_hdmi = dai_to_hdmi(dai);
+	struct vc4_hdmi *vc4_hdmi = dev_get_drvdata(dev);
 	struct drm_encoder *encoder = &vc4_hdmi->encoder.base.base;
-	struct drm_connector *connector = &vc4_hdmi->connector;
-	int ret;
-
-	if (vc4_hdmi->audio.substream && vc4_hdmi->audio.substream != substream)
-		return -EINVAL;
-
-	vc4_hdmi->audio.substream = substream;
 
 	/*
 	 * If the HDMI encoder hasn't probed, or the encoder is
@@ -1235,15 +1228,18 @@ static int vc4_hdmi_audio_startup(struct
 				VC4_HDMI_RAM_PACKET_ENABLE))
 		return -ENODEV;
 
-	ret = snd_pcm_hw_constraint_eld(substream->runtime, connector->eld);
-	if (ret)
-		return ret;
+	vc4_hdmi->audio.streaming = true;
 
-	return 0;
-}
+	HDMI_WRITE(HDMI_MAI_CTL,
+		   VC4_HD_MAI_CTL_RESET |
+		   VC4_HD_MAI_CTL_FLUSH |
+		   VC4_HD_MAI_CTL_DLATE |
+		   VC4_HD_MAI_CTL_ERRORE |
+		   VC4_HD_MAI_CTL_ERRORF);
+
+	if (vc4_hdmi->variant->phy_rng_enable)
+		vc4_hdmi->variant->phy_rng_enable(vc4_hdmi);
 
-static int vc4_hdmi_audio_set_fmt(struct snd_soc_dai *dai, unsigned int fmt)
-{
 	return 0;
 }
 
@@ -1263,17 +1259,20 @@ static void vc4_hdmi_audio_reset(struct
 	HDMI_WRITE(HDMI_MAI_CTL, VC4_HD_MAI_CTL_FLUSH);
 }
 
-static void vc4_hdmi_audio_shutdown(struct snd_pcm_substream *substream,
-				    struct snd_soc_dai *dai)
+static void vc4_hdmi_audio_shutdown(struct device *dev, void *data)
 {
-	struct vc4_hdmi *vc4_hdmi = dai_to_hdmi(dai);
+	struct vc4_hdmi *vc4_hdmi = dev_get_drvdata(dev);
 
-	if (substream != vc4_hdmi->audio.substream)
-		return;
+	HDMI_WRITE(HDMI_MAI_CTL,
+		   VC4_HD_MAI_CTL_DLATE |
+		   VC4_HD_MAI_CTL_ERRORE |
+		   VC4_HD_MAI_CTL_ERRORF);
 
-	vc4_hdmi_audio_reset(vc4_hdmi);
+	if (vc4_hdmi->variant->phy_rng_disable)
+		vc4_hdmi->variant->phy_rng_disable(vc4_hdmi);
 
-	vc4_hdmi->audio.substream = NULL;
+	vc4_hdmi->audio.streaming = false;
+	vc4_hdmi_audio_reset(vc4_hdmi);
 }
 
 static int sample_rate_to_mai_fmt(int samplerate)
@@ -1315,42 +1314,35 @@ static int sample_rate_to_mai_fmt(int sa
 }
 
 /* HDMI audio codec callbacks */
-static int vc4_hdmi_audio_prepare(struct snd_pcm_substream *substream,
-				  struct snd_soc_dai *dai)
+static int vc4_hdmi_audio_prepare(struct device *dev, void *data,
+				  struct hdmi_codec_daifmt *daifmt,
+				  struct hdmi_codec_params *params)
 {
-	struct vc4_hdmi *vc4_hdmi = dai_to_hdmi(dai);
+	struct vc4_hdmi *vc4_hdmi = dev_get_drvdata(dev);
 	struct drm_encoder *encoder = &vc4_hdmi->encoder.base.base;
-	struct device *dev = &vc4_hdmi->pdev->dev;
 	u32 audio_packet_config, channel_mask;
 	u32 channel_map;
 	u32 mai_audio_format;
 	u32 mai_sample_rate;
 
-	if (substream != vc4_hdmi->audio.substream)
-		return -EINVAL;
+	dev_dbg(dev, "%s: %u Hz, %d bit, %d channels\n", __func__,
+		params->sample_rate, params->sample_width,
+		params->channels);
 
-	dev_dbg(dev, "%s: %u Hz, %d bit, %d channels AES0=%02x\n",
-		__func__,
-		substream->runtime->rate,
-		snd_pcm_format_width(substream->runtime->format),
-		substream->runtime->channels,
-		vc4_hdmi->audio.iec_status[0]);
-
-	vc4_hdmi->audio.channels = substream->runtime->channels;
-	vc4_hdmi->audio.samplerate = substream->runtime->rate;
+	vc4_hdmi->audio.channels = params->channels;
+	vc4_hdmi->audio.samplerate = params->sample_rate;
 
 	HDMI_WRITE(HDMI_MAI_CTL,
-		   VC4_HD_MAI_CTL_RESET |
-		   VC4_HD_MAI_CTL_FLUSH |
-		   VC4_HD_MAI_CTL_DLATE |
-		   VC4_HD_MAI_CTL_ERRORE |
-		   VC4_HD_MAI_CTL_ERRORF);
+		   VC4_SET_FIELD(params->channels, VC4_HD_MAI_CTL_CHNUM) |
+		   VC4_HD_MAI_CTL_WHOLSMP |
+		   VC4_HD_MAI_CTL_CHALIGN |
+		   VC4_HD_MAI_CTL_ENABLE);
 
 	vc4_hdmi_audio_set_mai_clock(vc4_hdmi);
 
 	mai_sample_rate = sample_rate_to_mai_fmt(vc4_hdmi->audio.samplerate);
-	if (vc4_hdmi->audio.iec_status[0] & IEC958_AES0_NONAUDIO &&
-	    vc4_hdmi->audio.channels == 8)
+	if (params->iec.status[0] & IEC958_AES0_NONAUDIO &&
+	    params->channels == 8)
 		mai_audio_format = VC4_HDMI_MAI_FORMAT_HBR;
 	else
 		mai_audio_format = VC4_HDMI_MAI_FORMAT_PCM;
@@ -1387,148 +1379,12 @@ static int vc4_hdmi_audio_prepare(struct
 	HDMI_WRITE(HDMI_AUDIO_PACKET_CONFIG, audio_packet_config);
 	vc4_hdmi_set_n_cts(vc4_hdmi);
 
+	memcpy(&vc4_hdmi->audio.infoframe, &params->cea, sizeof(params->cea));
 	vc4_hdmi_set_audio_infoframe(encoder);
 
 	return 0;
 }
 
-static int vc4_hdmi_audio_trigger(struct snd_pcm_substream *substream, int cmd,
-				  struct snd_soc_dai *dai)
-{
-	struct vc4_hdmi *vc4_hdmi = dai_to_hdmi(dai);
-
-	switch (cmd) {
-	case SNDRV_PCM_TRIGGER_START:
-		vc4_hdmi->audio.streaming = true;
-
-		if (vc4_hdmi->variant->phy_rng_enable)
-			vc4_hdmi->variant->phy_rng_enable(vc4_hdmi);
-
-		HDMI_WRITE(HDMI_MAI_CTL,
-			   VC4_SET_FIELD(vc4_hdmi->audio.channels,
-					 VC4_HD_MAI_CTL_CHNUM) |
-					 VC4_HD_MAI_CTL_WHOLSMP |
-					 VC4_HD_MAI_CTL_CHALIGN |
-					 VC4_HD_MAI_CTL_ENABLE);
-		break;
-	case SNDRV_PCM_TRIGGER_STOP:
-		HDMI_WRITE(HDMI_MAI_CTL,
-			   VC4_HD_MAI_CTL_DLATE |
-			   VC4_HD_MAI_CTL_ERRORE |
-			   VC4_HD_MAI_CTL_ERRORF);
-
-		if (vc4_hdmi->variant->phy_rng_disable)
-			vc4_hdmi->variant->phy_rng_disable(vc4_hdmi);
-
-		vc4_hdmi->audio.streaming = false;
-
-		break;
-	default:
-		break;
-	}
-
-	return 0;
-}
-
-static inline struct vc4_hdmi *
-snd_component_to_hdmi(struct snd_soc_component *component)
-{
-	struct snd_soc_card *card = snd_soc_component_get_drvdata(component);
-
-	return snd_soc_card_get_drvdata(card);
-}
-
-static int vc4_hdmi_audio_eld_ctl_info(struct snd_kcontrol *kcontrol,
-				       struct snd_ctl_elem_info *uinfo)
-{
-	struct snd_soc_component *component = snd_kcontrol_chip(kcontrol);
-	struct vc4_hdmi *vc4_hdmi = snd_component_to_hdmi(component);
-	struct drm_connector *connector = &vc4_hdmi->connector;
-
-	uinfo->type = SNDRV_CTL_ELEM_TYPE_BYTES;
-	uinfo->count = sizeof(connector->eld);
-
-	return 0;
-}
-
-static int vc4_hdmi_audio_eld_ctl_get(struct snd_kcontrol *kcontrol,
-				      struct snd_ctl_elem_value *ucontrol)
-{
-	struct snd_soc_component *component = snd_kcontrol_chip(kcontrol);
-	struct vc4_hdmi *vc4_hdmi = snd_component_to_hdmi(component);
-	struct drm_connector *connector = &vc4_hdmi->connector;
-
-	memcpy(ucontrol->value.bytes.data, connector->eld,
-	       sizeof(connector->eld));
-
-	return 0;
-}
-
-static int vc4_spdif_info(struct snd_kcontrol *kcontrol,
-			  struct snd_ctl_elem_info *uinfo)
-{
-	uinfo->type = SNDRV_CTL_ELEM_TYPE_IEC958;
-	uinfo->count = 1;
-	return 0;
-}
-
-static int vc4_spdif_playback_get(struct snd_kcontrol *kcontrol,
-				  struct snd_ctl_elem_value *ucontrol)
-{
-	struct snd_soc_component *component = snd_kcontrol_chip(kcontrol);
-	struct vc4_hdmi *vc4_hdmi = snd_component_to_hdmi(component);
-
-	memcpy(ucontrol->value.iec958.status, vc4_hdmi->audio.iec_status,
-	       sizeof(vc4_hdmi->audio.iec_status));
-
-	return 0;
-}
-
-static int vc4_spdif_playback_put(struct snd_kcontrol *kcontrol,
-				  struct snd_ctl_elem_value *ucontrol)
-{
-	struct snd_soc_component *component = snd_kcontrol_chip(kcontrol);
-	struct vc4_hdmi *vc4_hdmi = snd_component_to_hdmi(component);
-
-	memcpy(vc4_hdmi->audio.iec_status, ucontrol->value.iec958.status,
-	       sizeof(vc4_hdmi->audio.iec_status));
-
-	return 0;
-}
-
-static int vc4_spdif_mask_get(struct snd_kcontrol *kcontrol,
-			      struct snd_ctl_elem_value *ucontrol)
-{
-	memset(ucontrol->value.iec958.status, 0xff,
-	       sizeof_field(struct vc4_hdmi_audio, iec_status));
-
-	return 0;
-}
-
-static const struct snd_kcontrol_new vc4_hdmi_audio_controls[] = {
-	{
-		.access = SNDRV_CTL_ELEM_ACCESS_READ |
-			  SNDRV_CTL_ELEM_ACCESS_VOLATILE,
-		.iface = SNDRV_CTL_ELEM_IFACE_PCM,
-		.name = "ELD",
-		.info = vc4_hdmi_audio_eld_ctl_info,
-		.get = vc4_hdmi_audio_eld_ctl_get,
-	},
-	{
-		.iface =   SNDRV_CTL_ELEM_IFACE_MIXER,
-		.name =    SNDRV_CTL_NAME_IEC958("", PLAYBACK, DEFAULT),
-		.info =    vc4_spdif_info,
-		.get =     vc4_spdif_playback_get,
-		.put =     vc4_spdif_playback_put,
-	},
-	{
-		.iface =   SNDRV_CTL_ELEM_IFACE_MIXER,
-		.name =    SNDRV_CTL_NAME_IEC958("", PLAYBACK, MASK),
-		.info =    vc4_spdif_info,
-		.get =     vc4_spdif_mask_get,
-	},
-};
-
 static const struct snd_soc_dapm_widget vc4_hdmi_audio_widgets[] = {
 	SND_SOC_DAPM_OUTPUT("TX"),
 };
@@ -1539,8 +1395,6 @@ static const struct snd_soc_dapm_route v
 
 static const struct snd_soc_component_driver vc4_hdmi_audio_component_drv = {
 	.name			= "vc4-hdmi-codec-dai-component",
-	.controls		= vc4_hdmi_audio_controls,
-	.num_controls		= ARRAY_SIZE(vc4_hdmi_audio_controls),
 	.dapm_widgets		= vc4_hdmi_audio_widgets,
 	.num_dapm_widgets	= ARRAY_SIZE(vc4_hdmi_audio_widgets),
 	.dapm_routes		= vc4_hdmi_audio_routes,
@@ -1551,28 +1405,6 @@ static const struct snd_soc_component_dr
 	.non_legacy_dai_naming	= 1,
 };
 
-static const struct snd_soc_dai_ops vc4_hdmi_audio_dai_ops = {
-	.startup = vc4_hdmi_audio_startup,
-	.shutdown = vc4_hdmi_audio_shutdown,
-	.prepare = vc4_hdmi_audio_prepare,
-	.set_fmt = vc4_hdmi_audio_set_fmt,
-	.trigger = vc4_hdmi_audio_trigger,
-};
-
-static struct snd_soc_dai_driver vc4_hdmi_audio_codec_dai_drv = {
-	.name = "vc4-hdmi-hifi",
-	.playback = {
-		.stream_name = "Playback",
-		.channels_min = 2,
-		.channels_max = 8,
-		.rates = SNDRV_PCM_RATE_32000 | SNDRV_PCM_RATE_44100 |
-			 SNDRV_PCM_RATE_48000 | SNDRV_PCM_RATE_88200 |
-			 SNDRV_PCM_RATE_96000 | SNDRV_PCM_RATE_176400 |
-			 SNDRV_PCM_RATE_192000,
-		.formats = SNDRV_PCM_FMTBIT_IEC958_SUBFRAME_LE,
-	},
-};
-
 static const struct snd_soc_component_driver vc4_hdmi_audio_cpu_dai_comp = {
 	.name = "vc4-hdmi-cpu-dai-component",
 };
@@ -1599,7 +1431,6 @@ static struct snd_soc_dai_driver vc4_hdm
 			 SNDRV_PCM_RATE_192000,
 		.formats = SNDRV_PCM_FMTBIT_IEC958_SUBFRAME_LE,
 	},
-	.ops = &vc4_hdmi_audio_dai_ops,
 };
 
 static const struct snd_dmaengine_pcm_config pcm_conf = {
@@ -1607,6 +1438,31 @@ static const struct snd_dmaengine_pcm_co
 	.prepare_slave_config = snd_dmaengine_pcm_prepare_slave_config,
 };
 
+
+static int vc4_hdmi_audio_get_eld(struct device *dev, void *data,
+				  uint8_t *buf, size_t len)
+{
+	struct vc4_hdmi *vc4_hdmi = dev_get_drvdata(dev);
+	struct drm_connector *connector = &vc4_hdmi->connector;
+
+	memcpy(buf, connector->eld, min(sizeof(connector->eld), len));
+
+	return 0;
+}
+
+static const struct hdmi_codec_ops vc4_hdmi_codec_ops = {
+	.get_eld = vc4_hdmi_audio_get_eld,
+	.prepare = vc4_hdmi_audio_prepare,
+	.audio_shutdown = vc4_hdmi_audio_shutdown,
+	.audio_startup = vc4_hdmi_audio_startup,
+};
+
+struct hdmi_codec_pdata vc4_hdmi_codec_pdata = {
+	.ops = &vc4_hdmi_codec_ops,
+	.max_i2s_channels = 8,
+	.i2s = 1,
+};
+
 static int vc4_hdmi_audio_init(struct vc4_hdmi *vc4_hdmi)
 {
 	const struct vc4_hdmi_register *mai_data =
@@ -1614,6 +1470,7 @@ static int vc4_hdmi_audio_init(struct vc
 	struct snd_soc_dai_link *dai_link = &vc4_hdmi->audio.link;
 	struct snd_soc_card *card = &vc4_hdmi->audio.card;
 	struct device *dev = &vc4_hdmi->pdev->dev;
+	struct platform_device *codec_pdev;
 	const __be32 *addr;
 	int index;
 	int ret;
@@ -1649,11 +1506,6 @@ static int vc4_hdmi_audio_init(struct vc
 	vc4_hdmi->audio.dma_data.addr_width = DMA_SLAVE_BUSWIDTH_4_BYTES;
 	vc4_hdmi->audio.dma_data.maxburst = 2;
 
-	vc4_hdmi->audio.iec_status[0] = IEC958_AES0_CON_NOT_COPYRIGHT;
-	vc4_hdmi->audio.iec_status[1] =
-		IEC958_AES1_CON_ORIGINAL | IEC958_AES1_CON_PCM_CODER;
-	vc4_hdmi->audio.iec_status[3] = IEC958_AES3_CON_FS_48000;
-
 	ret = devm_snd_dmaengine_pcm_register(dev, &pcm_conf, 0);
 	if (ret) {
 		dev_err(dev, "Could not register PCM component: %d\n", ret);
@@ -1667,12 +1519,13 @@ static int vc4_hdmi_audio_init(struct vc
 		return ret;
 	}
 
-	/* register component and codec dai */
-	ret = devm_snd_soc_register_component(dev, &vc4_hdmi_audio_component_drv,
-				     &vc4_hdmi_audio_codec_dai_drv, 1);
-	if (ret) {
-		dev_err(dev, "Could not register component: %d\n", ret);
-		return ret;
+	codec_pdev = platform_device_register_data(dev, HDMI_CODEC_DRV_NAME,
+						   PLATFORM_DEVID_AUTO,
+						   &vc4_hdmi_codec_pdata,
+						   sizeof(vc4_hdmi_codec_pdata));
+	if (IS_ERR(codec_pdev)) {
+		dev_err(dev, "Couldn't register the HDMI codec: %ld\n", PTR_ERR(codec_pdev));
+		return PTR_ERR(codec_pdev);
 	}
 
 	dai_link->cpus		= &vc4_hdmi->audio.cpu;
@@ -1685,9 +1538,9 @@ static int vc4_hdmi_audio_init(struct vc
 
 	dai_link->name = "MAI";
 	dai_link->stream_name = "MAI PCM";
-	dai_link->codecs->dai_name = vc4_hdmi_audio_codec_dai_drv.name;
+	dai_link->codecs->dai_name = "i2s-hifi";
 	dai_link->cpus->dai_name = dev_name(dev);
-	dai_link->codecs->name = dev_name(dev);
+	dai_link->codecs->name = dev_name(&codec_pdev->dev);
 	dai_link->platforms->name = dev_name(dev);
 
 	card->dai_link = dai_link;
--- a/drivers/gpu/drm/vc4/vc4_hdmi.h
+++ b/drivers/gpu/drm/vc4/vc4_hdmi.h
@@ -114,8 +114,7 @@ struct vc4_hdmi_audio {
 	int samplerate;
 	int channels;
 	struct snd_dmaengine_dai_dma_data dma_data;
-	struct snd_pcm_substream *substream;
-
+	struct hdmi_audio_infoframe infoframe;
 	bool streaming;
 
 	unsigned char iec_status[4];
