From aac689d308b3f6dff8a8ccbd85f8a32078a92318 Mon Sep 17 00:00:00 2001
From: Martin Sperl <kernel@martin.sperl.org>
Date: Mon, 13 May 2019 11:05:27 +0000
Subject: [PATCH] spi: bcm2835: enable shared interrupt support

Add shared interrupt support for this driver.

Signed-off-by: Martin Sperl <kernel@martin.sperl.org>
---
 drivers/spi/spi-bcm2835.c | 7 ++++++-
 1 file changed, 6 insertions(+), 1 deletion(-)

--- a/drivers/spi/spi-bcm2835.c
+++ b/drivers/spi/spi-bcm2835.c
@@ -379,6 +379,10 @@ static irqreturn_t bcm2835_spi_interrupt
 	if (bs->tx_len && cs & BCM2835_SPI_CS_DONE)
 		bcm2835_wr_fifo_blind(bs, BCM2835_SPI_FIFO_SIZE);
 
+	/* check if we got interrupt enabled */
+	if (!(bcm2835_rd(bs, BCM2835_SPI_CS) & BCM2835_SPI_CS_INTR))
+		return IRQ_NONE;
+
 	/* Read as many bytes as possible from FIFO */
 	bcm2835_rd_fifo(bs);
 	/* Write as many bytes as possible to FIFO */
@@ -1329,7 +1333,8 @@ static int bcm2835_spi_probe(struct plat
 	bcm2835_wr(bs, BCM2835_SPI_CS,
 		   BCM2835_SPI_CS_CLEAR_RX | BCM2835_SPI_CS_CLEAR_TX);
 
-	err = devm_request_irq(&pdev->dev, bs->irq, bcm2835_spi_interrupt, 0,
+	err = devm_request_irq(&pdev->dev, bs->irq, bcm2835_spi_interrupt,
+			       IRQF_SHARED,
 			       dev_name(&pdev->dev), bs);
 	if (err) {
 		dev_err(&pdev->dev, "could not request IRQ: %d\n", err);
