#include "ar9.dtsi"

#include <dt-bindings/input/input.h>

/ {
	compatible = "zte,h201l", "lantiq,xway", "lantiq,ar9";
	model = "ZTE H210L";

	chosen {
		bootargs = "console=ttyLTQ0,115200";
	};

	aliases {
		led-boot = &power_green;
		led-failsafe = &power_green;
		led-running = &power_green;
		led-upgrade = &power_green;

		led-dsl = &dsl;
		led-internet = &online;
		led-usb = &led_usb;
		led-wifi = &wifi;
	};

	memory@0 {
		device_type = "memory";
		reg = <0x0 0x2000000>;
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <100>;

		reset {
			label = "reset";
			gpios = <&gpio 53 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
		wps {
			label = "wps";
			gpios = <&gpio 54 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};
		rfkill {
			label = "rfkill";
			gpios = <&gpio 55 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RFKILL>;
		};
	};

	leds {
		compatible = "gpio-leds";

		power_green: power {
			label = "green:power";
			gpios = <&gpio 19 GPIO_ACTIVE_LOW>;
			default-state = "keep";
		};
		online: online {
			label = "green:internet";
			gpios = <&gpio 37 GPIO_ACTIVE_LOW>;
		};
		dsl: dsl {
			label = "green:dsl";
			gpios = <&gpio 4 GPIO_ACTIVE_LOW>;
		};
		phone {
			label = "green:phone";
			gpios = <&gpio 39 GPIO_ACTIVE_LOW>;
		};
		wps {
			label = "green:wps";
			gpios = <&gpio 22 GPIO_ACTIVE_LOW>;
		};
		wifi: wifi {
			label = "green:wlan";
			gpios = <&gpio 6 GPIO_ACTIVE_LOW>;
		};
		led_usb: usb {
			label = "green:usb";
			gpios = <&gpio 14 GPIO_ACTIVE_LOW>;
		};
	};

	gpio_export {
		compatible = "gpio-export";
		#size-cells = <0>;

		switch {
			gpio-export,name = "switch";
			gpio-export,output = <1>;
			gpios = <&gpio 38 GPIO_ACTIVE_HIGH>;
		};
		usb {
			gpio-export,name = "usb";
			gpio-export,output = <1>;
			gpios = <&gpio 28 GPIO_ACTIVE_HIGH>;
		};
		wifi {
			gpio-export,name = "wifi";
			gpio-export,output = <1>;
			gpios = <&gpio 7 GPIO_ACTIVE_HIGH>;
		};
	};

	usb_vbus: regulator-usb-vbus {
		compatible = "regulator-fixed";

		regulator-name = "USB_VBUS";

		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;

		gpio = <&gpio 36 GPIO_ACTIVE_HIGH>;
		enable-active-high;
	};
};

&gpio {
	pinctrl-names = "default";
	pinctrl-0 = <&state_default>;

	state_default: pinmux {
	};
};

&gsw {
	phy-mode = "rgmii";
};

&localbus {
	flash@0 {
		compatible = "lantiq,nor";
		bank-width = <2>;
		reg = <0 0x0 0x2000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "uboot";
				reg = <0x00000 0x20000>;
				read-only;
			};

			partition@20000 {
				label = "u-boot-env";
				reg = <0x20000 0x10000>;
				read-only;
			};

			partition@30000 {
				label = "firmware";
				reg = <0x30000 0x7d0000>;
			};
		};
	};
};

&usb_phy0 {
	status = "okay";
};


&usb0 {
	status = "okay";
	vbus-supply = <&usb_vbus>;
};
