From c17702bad18a085ae913752b45bcc20c2cea879e Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?=C3=81lvaro=20Fern=C3=A1ndez=20Rojas?= <noltari@gmail.com>
Date: Thu, 25 Feb 2021 19:53:08 +0100
Subject: [PATCH 3/4] dt-bindings: clock: Add BCM63268 timer binding
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Document the Broadcom BCM63268 Clock and Reset controller.

Signed-off-by: Álvaro Fernández Rojas <noltari@gmail.com>
---
 .../clock/brcm,bcm63268-timer-clocks.yaml     | 40 +++++++++++++++++++
 1 file changed, 40 insertions(+)
 create mode 100644 Documentation/devicetree/bindings/clock/brcm,bcm63268-timer-clocks.yaml

--- /dev/null
+++ b/Documentation/devicetree/bindings/clock/brcm,bcm63268-timer-clocks.yaml
@@ -0,0 +1,40 @@
+# SPDX-License-Identifier: (GPL-2.0-only OR BSD-2-Clause)
+%YAML 1.2
+---
+$id: http://devicetree.org/schemas/clock/brcm,bcm63268-timer-clocks.yaml#
+$schema: http://devicetree.org/meta-schemas/core.yaml#
+
+title: Broadcom BCM63268 Timer Clock and Reset Device Tree Bindings
+
+maintainers:
+  - Álvaro Fernández Rojas <noltari@gmail.com>
+
+properties:
+  compatible:
+    const: brcm,bcm63268-timer-clocks
+
+  reg:
+    maxItems: 1
+
+  "#clock-cells":
+    const: 1
+
+  "#reset-cells":
+    const: 1
+
+required:
+  - compatible
+  - reg
+  - "#clock-cells"
+  - "#reset-cells"
+
+additionalProperties: false
+
+examples:
+  - |
+    timer_clk: clock-controller@100000ac {
+      compatible = "brcm,bcm63268-timer-clocks";
+      reg = <0x100000ac 0x4>;
+      #clock-cells = <1>;
+      #reset-cells = <1>;
+    };
