// SPDX-License-Identifier: GPL-2.0-only

#include "mt7621.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "mediatek,mt7621-soc";

	aliases {
		label-mac-device = &gmac0;
		led-boot = &led_power_white;
		led-failsafe = &led_power_orange;
		led-running = &led_power_white;
		led-upgrade = &led_power_orange;
	};

	keys {
		compatible = "gpio-keys";

		wps {
			label = "wps";
			gpios = <&gpio 18 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};

		rfkill {
			label = "rfkill";
			gpios = <&gpio 14 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RFKILL>;
		};

		reset {
			label = "reset";
			gpios = <&gpio 12 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};

	leds: leds {
		compatible = "gpio-leds";

		led_power_orange: power_orange {
			gpios = <&gpio_expander 0 GPIO_ACTIVE_LOW>;
			label = "orange:power";
		};

		led_power_white: power_white {
			gpios = <&gpio_expander 1 GPIO_ACTIVE_LOW>;
			label = "white:power";
		};

		wan_orange {
			gpios = <&gpio_expander 2 GPIO_ACTIVE_LOW>;
			label = "orange:wan";
		};

		wan_white {
			gpios = <&gpio_expander 3 GPIO_ACTIVE_LOW>;
			label = "white:wan";
		};

		wlan2g {
			gpios = <&gpio_expander 4 GPIO_ACTIVE_LOW>;
			label = "white:wlan2g";
			linux,default-trigger = "phy0radio";
		};

		wlan5g {
			gpios = <&gpio_expander 5 GPIO_ACTIVE_LOW>;
			label = "white:wlan5g";
			linux,default-trigger = "phy1radio";
		};

		usb3 {
			gpios = <&gpio_expander 7 GPIO_ACTIVE_LOW>;
			label = "white:usb3";
			linux,default-trigger = "usbport";
			trigger-sources = <&xhci_ehci_port1>;
		};

		lan1_orange {
			gpios = <&gpio_expander 8 GPIO_ACTIVE_LOW>;
			label = "orange:lan1";
		};

		lan1_white {
			gpios = <&gpio_expander 9 GPIO_ACTIVE_LOW>;
			label = "white:lan1";
		};

		lan2_orange {
			gpios = <&gpio_expander 10 GPIO_ACTIVE_LOW>;
			label = "orange:lan2";
		};

		lan2_white {
			gpios = <&gpio_expander 11 GPIO_ACTIVE_LOW>;
			label = "white:lan2";
		};

		lan3_orange {
			gpios = <&gpio_expander 12 GPIO_ACTIVE_LOW>;
			label = "orange:lan3";
		};

		lan3_white {
			gpios = <&gpio_expander 13 GPIO_ACTIVE_LOW>;
			label = "white:lan3";
		};

		lan4_orange {
			gpios = <&gpio_expander 14 GPIO_ACTIVE_LOW>;
			label = "orange:lan4";
		};

		lan4_white {
			gpios = <&gpio_expander 15 GPIO_ACTIVE_LOW>;
			label = "white:lan4";
		};

		wps {
			gpios = <&gpio 17 GPIO_ACTIVE_HIGH>;
			label = "white:wps";
		};

		wlan {
			gpios = <&gpio 5 GPIO_ACTIVE_LOW>;
			label = "white:wlan";
		};
	};
};

&state_default {
	gpio {
		groups = "uart3", "uart2", "jtag", "wdt";
		function = "gpio";
	};
};

&pcie {
	status = "okay";
};

&pcie0 {
	wifi@0,0 {
		compatible = "mediatek,mt76";
		reg = <0x0 0 0 0 0>;
		mediatek,mtd-eeprom = <&factory 0x0>;
		ieee80211-freq-limit = <2400000 2500000>;
	};
};

&pcie1 {
	wifi@0,0 {
		compatible = "mediatek,mt76";
		reg = <0x0 0 0 0 0>;
		mediatek,mtd-eeprom = <&factory 0x8000>;
		ieee80211-freq-limit = <5000000 6000000>;
	};
};

&gmac0 {
	nvmem-cells = <&macaddr_factory_4>;
	nvmem-cell-names = "mac-address";
};

&switch0 {
	ports {
		port@0 {
			status = "okay";
			label = "lan4";
		};

		port@1 {
			status = "okay";
			label = "lan3";
		};

		port@2 {
			status = "okay";
			label = "lan2";
		};

		port@3 {
			status = "okay";
			label = "lan1";
		};

		port@4 {
			status = "okay";
			label = "wan";
			nvmem-cells = <&macaddr_factory_4>;
			nvmem-cell-names = "mac-address";
			mac-address-increment = <2>;
		};
	};
};

&i2c {
	status = "okay";

	gpio_expander: i2c0gpio-expander@20{
		#gpio-cells = <2>;
		#interrupt-cells = <2>;
		compatible = "semtech,sx1503q";
		reg = <0x20>;

		gpio-controller;
	};
};

&nand {
	status = "okay";

	partitions {
		compatible = "fixed-partitions";
		#address-cells = <1>;
		#size-cells = <1>;

		partition@0 {
			label = "u-boot";
			reg = <0x0 0x100000>;
			read-only;
		};

		partition@100000 {
			label = "SC PART_MAP";
			reg = <0x100000 0x100000>;
			read-only;
		};

		partition@200000 {
			label = "kernel";
			reg = <0x200000 0x400000>;
		};

		partition@600000 {
			label = "ubi";
			reg = <0x600000 0x2800000>;
		};

		partition@2e00000 {
			label = "reserved0";
			reg = <0x2e00000 0x1800000>;
			read-only;
		};

		factory: partition@4600000 {
			label = "factory";
			reg = <0x4600000 0x200000>;
			read-only;
		};

		partition@4800000 {
			label = "reserved1";
			reg = <0x4800000 0x3800000>;
			read-only;
		};
	};
};

&factory {
	compatible = "nvmem-cells";
	#address-cells = <1>;
	#size-cells = <1>;

	macaddr_factory_4: macaddr@4 {
		reg = <0x4 0x6>;
	};
};
