From e2e8b2dfdfda27958a276c719fda8b162f229bc8 Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.com>
Date: Tue, 21 Jul 2020 17:34:09 +0100
Subject: [PATCH] staging: vchiq_arm: children inherit DMA config

Although it is no longer necessary for vchiq's children to have a
different DMA configuration to the parent, they do still need to
explicitly to have their DMA configuration set - to be that of the
parent.

Signed-off-by: Phil Elwell <phil@raspberrypi.com>
---
 .../vc04_services/interface/vchiq_arm/vchiq_arm.c      | 10 ++++++++++
 1 file changed, 10 insertions(+)

--- a/drivers/staging/vc04_services/interface/vchiq_arm/vchiq_arm.c
+++ b/drivers/staging/vc04_services/interface/vchiq_arm/vchiq_arm.c
@@ -2720,8 +2720,18 @@ vchiq_register_child(struct platform_dev
 
 	child->dev.of_node = np;
 
+	/*
+	 * We want the dma-ranges etc to be copied from the parent VCHIQ device
+	 * to be passed on to the children without a node of their own.
+	 */
+	if (!np)
+		np = pdev->dev.of_node;
+
 	of_dma_configure(&child->dev, np, true);
 
+	if (np != pdev->dev.of_node)
+		of_node_put(np);
+
 	return child;
 }
 
