From f4980947debc7865bd923d60bf36d6fb0b80ecc5 Mon Sep 17 00:00:00 2001
From: Xiaowei Bao <xiaowei.bao@nxp.com>
Date: Fri, 23 Aug 2019 16:26:43 +0800
Subject: [PATCH] PCI: layerscape: Add LS1028a support

Add support for the LS1028a PCIe controller.

Signed-off-by: Xiaowei Bao <xiaowei.bao@nxp.com>
Signed-off-by: Hou Zhiqiang <Zhiqiang.Hou@nxp.com>
---
 drivers/pci/controller/dwc/pci-layerscape.c | 1 +
 1 file changed, 1 insertion(+)

--- a/drivers/pci/controller/dwc/pci-layerscape.c
+++ b/drivers/pci/controller/dwc/pci-layerscape.c
@@ -263,6 +263,7 @@ static const struct ls_pcie_drvdata ls20
 static const struct of_device_id ls_pcie_of_match[] = {
 	{ .compatible = "fsl,ls1012a-pcie", .data = &ls1046_drvdata },
 	{ .compatible = "fsl,ls1021a-pcie", .data = &ls1021_drvdata },
+	{ .compatible = "fsl,ls1028a-pcie", .data = &ls2088_drvdata },
 	{ .compatible = "fsl,ls1043a-pcie", .data = &ls1043_drvdata },
 	{ .compatible = "fsl,ls1046a-pcie", .data = &ls1046_drvdata },
 	{ .compatible = "fsl,ls2080a-pcie", .data = &ls2080_drvdata },
