// SPDX-License-Identifier: BSD-3-Clause
/*
 *  Copyright (C) 2018 Piotr Dymacz <pepe2k@gmail.com>
 *  All rights reserved.
 */

#include "mt7628an.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "alfa-network,awusfree1", "mediatek,mt7628an-soc";
	model = "ALFA Network AWUSFREE1";

	aliases {
		led-boot = &led_system;
		led-failsafe = &led_system;
		led-running = &led_system;
		led-upgrade = &led_system;
	};

	chosen {
		bootargs = "console=ttyS0,115200";
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			gpios = <&gpio 38 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_system: system {
			label = "orange:system";
			gpios = <&gpio 43 GPIO_ACTIVE_LOW>;
		};

		wlan {
			label = "blue:wlan";
			gpios = <&gpio 44 GPIO_ACTIVE_LOW>;
		};
	};
};

&ehci {
	status = "disabled";
};

&esw {
	mediatek,portdisable = <0x1e>;
};

&ethernet {
	nvmem-cells = <&macaddr_factory_2e>;
	nvmem-cell-names = "mac-address";
};

&ohci {
	status = "disabled";
};

&state_default {
	gpio {
		groups = "p0led_an", "wdt", "wled_an";
		function = "gpio";
	};

	ext_lna {
		groups = "uart1";
		function = "sw_r";
	};

	ext_pa {
		groups = "i2s";
		function = "antenna";
	};
};

&spi0 {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <10000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x0 0x30000>;
				read-only;
			};

			partition@30000 {
				label = "u-boot-env";
				reg = <0x30000 0x1000>;
			};

			partition@31000 {
				label = "config";
				reg = <0x31000 0xf000>;
				read-only;
			};

			factory: partition@40000 {
				label = "factory";
				reg = <0x40000 0x10000>;
				read-only;
			};

			partition@50000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x50000 0x7b0000>;
			};
		};
	};
};

&wmac {
	status = "okay";

	mediatek,mtd-eeprom = <&factory 0x0>;
};

&factory {
	compatible = "nvmem-cells";
	#address-cells = <1>;
	#size-cells = <1>;

	macaddr_factory_2e: macaddr@2e {
		reg = <0x2e 0x6>;
	};
};
