From e0fa88eaa3c176b71e563da68949ac2ab45aaa61 Mon Sep 17 00:00:00 2001
From: Robert Marko <robert.marko@sartura.hr>
Date: Fri, 2 Oct 2020 10:43:26 +0200
Subject: [PATCH] arm: dts: ipq4019: QCA807x properties

This adds necessary DT properties for QCA807x PHY-s to IPQ4019 DTSI.

Signed-off-by: Robert Marko <robert.marko@sartura.hr>
---
 arch/arm/boot/dts/qcom-ipq4019.dtsi | 18 ++++++++++++++++++
 1 file changed, 18 insertions(+)

--- a/arch/arm/boot/dts/qcom-ipq4019.dtsi
+++ b/arch/arm/boot/dts/qcom-ipq4019.dtsi
@@ -8,6 +8,7 @@
 #include <dt-bindings/clock/qcom,gcc-ipq4019.h>
 #include <dt-bindings/interrupt-controller/arm-gic.h>
 #include <dt-bindings/interrupt-controller/irq.h>
+#include <dt-bindings/net/qcom-qca807x.h>
 
 / {
 	#address-cells = <1>;
@@ -597,22 +598,39 @@
 
 			ethphy0: ethernet-phy@0 {
 				reg = <0>;
+
+				qcom,control-dac = <QCA807X_CONTROL_DAC_DSP_VOLT_QUARTER_BIAS>;
 			};
 
 			ethphy1: ethernet-phy@1 {
 				reg = <1>;
+
+				qcom,control-dac = <QCA807X_CONTROL_DAC_DSP_VOLT_QUARTER_BIAS>;
 			};
 
 			ethphy2: ethernet-phy@2 {
 				reg = <2>;
+
+				qcom,control-dac = <QCA807X_CONTROL_DAC_DSP_VOLT_QUARTER_BIAS>;
 			};
 
 			ethphy3: ethernet-phy@3 {
 				reg = <3>;
+
+				qcom,control-dac = <QCA807X_CONTROL_DAC_DSP_VOLT_QUARTER_BIAS>;
 			};
 
 			ethphy4: ethernet-phy@4 {
 				reg = <4>;
+
+				qcom,control-dac = <QCA807X_CONTROL_DAC_DSP_VOLT_QUARTER_BIAS>;
+			};
+
+			psgmiiphy: psgmii-phy@5 {
+				reg = <5>;
+
+				qcom,tx-driver-strength = <PSGMII_QSGMII_TX_DRIVER_300MV>;
+				qcom,psgmii-az;
 			};
 		};
 
